Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  Internet address is 10.100.0.238/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     27248 packets input, 2448864 bytes
     Received 1 broadcasts, 45 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     96599 packets output, 19383323 bytes
     Sent 3 broadcasts, 40114 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     14 packets input, 896 bytes
     Received 0 broadcasts, 14 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40127 packets output, 7258833 bytes
     Sent 0 broadcasts, 40127 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.0016 (bia 0021.0000.0016)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     11135146 packets input, 945521884 bytes
     Received 801479 broadcasts, 8034078 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     2339337 packets output, 248974681 bytes
     Sent 558 broadcasts, 40525 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.0017 (bia 0021.0000.0017)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     8836907 packets input, 704134618 bytes
     Received 801957 broadcasts, 8034437 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40922 packets output, 7318977 bytes
     Sent 0 broadcasts, 40914 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.0018 (bia 0021.0000.0018)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8836553 packets output, 700898383 bytes
     Sent 802006 broadcasts, 8034116 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.0019 (bia 0021.0000.0019)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8836546 packets output, 700897960 bytes
     Sent 802006 broadcasts, 8034109 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.001a (bia 0021.0000.001a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     2298827 packets input, 241684788 bytes
     Received 558 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     11135133 packets output, 942347174 bytes
     Sent 801448 broadcasts, 8034110 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:03:20 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     3 packets input, 192 bytes
     Received 0 broadcasts, 3 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40137 packets output, 7259518 bytes
     Sent 0 broadcasts, 40137 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     3 packets input, 192 bytes
     Received 0 broadcasts, 3 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40138 packets output, 7259574 bytes
     Sent 0 broadcasts, 40138 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40125 packets output, 7298940 bytes
     Sent 0 broadcasts, 40125 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0002.acc2
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 41 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40126 packets output, 7298996 bytes
     Sent 0 broadcasts, 40126 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.117.255.87/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 51 minutes, 6 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0021.0000.0011 (bia 0021.0000.0011)
  Internet address is 10.117.38.65/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 1 minutes, 48 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40099 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
