Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  Internet address is 10.100.0.216/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     39369 packets input, 3430642 bytes
     Received 1 broadcasts, 52 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     109702 packets output, 21784279 bytes
     Sent 0 broadcasts, 40116 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     259438 packets input, 207591832 bytes
     Received 2 broadcasts, 259271 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     179925 packets output, 192699697 bytes
     Sent 1 broadcasts, 179257 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0005.0027.29f1
  Internet address is 10.110.1.5/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 59 seconds
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     254882 packets input, 207305543 bytes
     Received 3 broadcasts, 254714 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     174974 packets output, 191779830 bytes
     Sent 0 broadcasts, 174806 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0005.0027.29f1
  Internet address is 10.110.1.1/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 59 seconds
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0000.0028 (bia 0005.0000.0028)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     250 packets input, 20788 bytes
     Received 1 broadcasts, 6 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     632628 packets output, 80073978 bytes
     Sent 3 broadcasts, 632261 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0000.002a (bia 0005.0000.002a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     253 packets input, 20980 bytes
     Received 1 broadcasts, 7 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     632630 packets output, 80074090 bytes
     Sent 3 broadcasts, 632263 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0000.002d (bia 0005.0000.002d)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     251 packets input, 20852 bytes
     Received 1 broadcasts, 6 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     632630 packets output, 80074082 bytes
     Sent 3 broadcasts, 632264 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0000.0030 (bia 0005.0000.0030)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     246 packets input, 20418 bytes
     Received 1 broadcasts, 6 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     632630 packets output, 80073999 bytes
     Sent 3 broadcasts, 632266 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40145 packets output, 7219820 bytes
     Sent 0 broadcasts, 40145 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40147 packets output, 7219932 bytes
     Sent 0 broadcasts, 40147 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     10 packets input, 640 bytes
     Received 0 broadcasts, 10 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40122 packets output, 7258750 bytes
     Sent 0 broadcasts, 40122 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     8 packets input, 512 bytes
     Received 0 broadcasts, 8 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40123 packets output, 7258681 bytes
     Sent 0 broadcasts, 40123 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet12 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     8 packets input, 512 bytes
     Received 0 broadcasts, 8 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40124 packets output, 7258737 bytes
     Sent 0 broadcasts, 40124 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet13 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40126 packets output, 7258849 bytes
     Sent 0 broadcasts, 40126 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet14 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40127 packets output, 7258905 bytes
     Sent 0 broadcasts, 40127 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet15 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40129 packets output, 7259017 bytes
     Sent 0 broadcasts, 40129 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet16 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:03:41 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40130 packets output, 7259073 bytes
     Sent 0 broadcasts, 40130 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet17 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40132 packets output, 7259185 bytes
     Sent 0 broadcasts, 40132 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40133 packets output, 7259241 bytes
     Sent 0 broadcasts, 40133 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet19 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0027.29f1
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 2 minutes, 57 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40136 packets output, 7259534 bytes
     Sent 0 broadcasts, 40136 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.10.4.3/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 51 minutes, 58 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0005.0000.001c (bia 0005.0000.001c)
  Internet address is 10.110.37.11/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 2 minutes, 37 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40095 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Vlan201 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0005.0027.29f1 (bia 0005.0027.29f1)
  Internet address is 10.101.10.1/25
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 59 seconds
