Physical interface: ge-0/0/0, Enabled, Physical link is Up
  Interface index: 139, SNMP ifIndex: 513
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:06, Hardware address: 00:07:00:00:00:06
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 72 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/0.0 (Index 329) (SNMP ifIndex 525)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 40105
    Output packets: 203817
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.100.0.52/31, Local: 10.100.0.52
    Protocol iso, MTU: 1497
      Flags: Is-Primary
    Protocol multiservice, MTU: Unlimited
      Flags: Is-Primary

Physical interface: lc-0/0/0, Enabled, Physical link is Up
  Interface index: 136, SNMP ifIndex: 507
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-0/0/0.32769 (Index 326) (SNMP ifIndex 508)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited
      Flags: Is-Primary

Physical interface: pfe-0/0/0, Enabled, Physical link is Up
  Interface index: 138, SNMP ifIndex: 511
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-0/0/0.16383 (Index 328) (SNMP ifIndex 512)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
      Flags: None

Physical interface: pfh-0/0/0, Enabled, Physical link is Up
  Interface index: 137, SNMP ifIndex: 509
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfh-0/0/0.16383 (Index 327) (SNMP ifIndex 510)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/1, Enabled, Physical link is Up
  Interface index: 140, SNMP ifIndex: 514
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:08, Hardware address: 00:07:00:00:00:08
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 448 bps (0 pps)
  Output rate    : 904 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/1.0 (Index 330) (SNMP ifIndex 539)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 966013
    Output packets: 1397011
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.16/30, Local: 10.10.1.18, Broadcast: 10.10.1.19
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
      Flags: Is-Primary
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/2, Enabled, Physical link is Up
  Interface index: 141, SNMP ifIndex: 515
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:0a, Hardware address: 00:07:00:00:00:0a
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 536 bps (0 pps)
  Output rate    : 840 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/2.0 (Index 331) (SNMP ifIndex 540)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 747083
    Output packets: 1270327
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.24/30, Local: 10.10.1.26, Broadcast: 10.10.1.27
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/3, Enabled, Physical link is Up
  Interface index: 142, SNMP ifIndex: 516
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:0c, Hardware address: 00:07:00:00:00:0c
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 920 bps (1 pps)
  Output rate    : 432 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/3.0 (Index 332) (SNMP ifIndex 541)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 1478066
    Output packets: 981564
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.0/30, Local: 10.10.1.2, Broadcast: 10.10.1.3
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/4, Enabled, Physical link is Up
  Interface index: 143, SNMP ifIndex: 517
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:0e, Hardware address: 00:07:00:00:00:0e
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 984 bps (1 pps)
  Output rate    : 528 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/4.0 (Index 333) (SNMP ifIndex 542)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 1260692
    Output packets: 850250
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.8/30, Local: 10.10.1.10, Broadcast: 10.10.1.11
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/5, Administratively down, Physical link is Down
  Interface index: 144, SNMP ifIndex: 518
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:0f, Hardware address: 00:07:00:00:00:0f
  Last flapped   : 2017-08-22 06:19:59 UTC (1w2d 15:36 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/5.0 (Index 334) (SNMP ifIndex 543)
    Flags: Device-Down SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 310317
    Output packets: 250760
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Dest-route-down Is-Preferred Is-Primary
        Destination: 10.10.1.32/30, Local: 10.10.1.34, Broadcast: 10.10.1.35
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/6, Administratively down, Physical link is Down
  Interface index: 145, SNMP ifIndex: 519
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:10, Hardware address: 00:07:00:00:00:10
  Last flapped   : 2017-08-22 06:19:59 UTC (1w2d 15:36 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/6.0 (Index 335) (SNMP ifIndex 544)
    Flags: Device-Down SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 310034
    Output packets: 250594
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Dest-route-down Is-Preferred Is-Primary
        Destination: 10.10.1.40/30, Local: 10.10.1.42, Broadcast: 10.10.1.43
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/7, Enabled, Physical link is Up
  Interface index: 146, SNMP ifIndex: 520
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:11, Hardware address: 00:07:00:00:00:11
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/8, Enabled, Physical link is Up
  Interface index: 147, SNMP ifIndex: 521
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:07:00:00:00:12, Hardware address: 00:07:00:00:00:12
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/9, Enabled, Physical link is Down
  Interface index: 148, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:09, Hardware address: 00:05:86:71:3f:09
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/10, Enabled, Physical link is Down
  Interface index: 149, SNMP ifIndex: 526
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0a, Hardware address: 00:05:86:71:3f:0a
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/11, Enabled, Physical link is Down
  Interface index: 150, SNMP ifIndex: 527
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0b, Hardware address: 00:05:86:71:3f:0b
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/12, Enabled, Physical link is Down
  Interface index: 151, SNMP ifIndex: 528
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0c, Hardware address: 00:05:86:71:3f:0c
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/13, Enabled, Physical link is Down
  Interface index: 152, SNMP ifIndex: 529
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0d, Hardware address: 00:05:86:71:3f:0d
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/14, Enabled, Physical link is Down
  Interface index: 153, SNMP ifIndex: 530
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0e, Hardware address: 00:05:86:71:3f:0e
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/15, Enabled, Physical link is Down
  Interface index: 154, SNMP ifIndex: 531
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:0f, Hardware address: 00:05:86:71:3f:0f
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/16, Enabled, Physical link is Down
  Interface index: 155, SNMP ifIndex: 532
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:10, Hardware address: 00:05:86:71:3f:10
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/17, Enabled, Physical link is Down
  Interface index: 156, SNMP ifIndex: 533
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:11, Hardware address: 00:05:86:71:3f:11
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/18, Enabled, Physical link is Down
  Interface index: 157, SNMP ifIndex: 534
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:12, Hardware address: 00:05:86:71:3f:12
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/19, Enabled, Physical link is Down
  Interface index: 158, SNMP ifIndex: 535
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:13, Hardware address: 00:05:86:71:3f:13
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/20, Enabled, Physical link is Down
  Interface index: 159, SNMP ifIndex: 536
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:14, Hardware address: 00:05:86:71:3f:14
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/21, Enabled, Physical link is Down
  Interface index: 160, SNMP ifIndex: 537
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:15, Hardware address: 00:05:86:71:3f:15
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/22, Enabled, Physical link is Down
  Interface index: 161, SNMP ifIndex: 538
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:3f:16, Hardware address: 00:05:86:71:3f:16
  Last flapped   : 2017-08-18 00:53:25 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ae0, Enabled, Physical link is Down
  Interface index: 128, SNMP ifIndex: 523
  Link-level type: Ethernet, MTU: 1514, Speed: Unspecified, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:42:c0, Hardware address: 00:05:86:71:42:c0
  Last flapped   : 2017-08-18 00:52:46 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)

Physical interface: ae1, Enabled, Physical link is Down
  Interface index: 129, SNMP ifIndex: 524
  Link-level type: Ethernet, MTU: 1514, Speed: Unspecified, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:42:c1, Hardware address: 00:05:86:71:42:c1
  Last flapped   : 2017-08-18 00:52:46 UTC (1w6d 21:03 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)

Physical interface: cbp0, Enabled, Physical link is Up
  Interface index: 131, SNMP ifIndex: 501
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:3f:11, Hardware address: 00:05:86:71:3f:11
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: demux0, Enabled, Physical link is Up
  Interface index: 130, SNMP ifIndex: 502
  Type: Software-Pseudo, MTU: 9192, Clocking: 1
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: dsc, Enabled, Physical link is Up
  Interface index: 5, SNMP ifIndex: 5
  Type: Software-Pseudo, MTU: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: em1, Enabled, Physical link is Up
  Interface index: 9, SNMP ifIndex: 23
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 52:54:00:01:43:8d, Hardware address: 52:54:00:01:43:8d
  Last flapped   : Never
    Input packets : 510991948
    Output packets: 570044025

  Logical interface em1.0 (Index 3) (SNMP ifIndex 24)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 510991940
    Output packets: 570044025
    Protocol inet, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 172.16/16, Local: 172.16.0.1, Broadcast: 172.16.255.255
    Protocol inet6, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred
        Destination: fe80::/64, Local: fe80::5254:ff:fe01:438d

Physical interface: fxp0, Enabled, Physical link is Up
  Interface index: 8, SNMP ifIndex: 1
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Current address: 00:07:00:00:00:15, Hardware address: 00:07:00:00:00:15
  Last flapped   : 2017-08-18 00:52:50 UTC (1w6d 21:03 ago)
    Input packets : 40661
    Output packets: 0

Physical interface: gre, Enabled, Physical link is Up
  Interface index: 10, SNMP ifIndex: 8
  Type: GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: ipip, Enabled, Physical link is Up
  Interface index: 11, SNMP ifIndex: 9
  Type: IPIP, Link-level type: IP-over-IP, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: irb, Enabled, Physical link is Up
  Interface index: 134, SNMP ifIndex: 503
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:42:f0, Hardware address: 00:05:86:71:42:f0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: lo0, Enabled, Physical link is Up
  Interface index: 6, SNMP ifIndex: 6
  Type: Loopback, MTU: Unlimited
  Device flags   : Present Running Loopback
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 4047
    Output packets: 4047

  Logical interface lo0.0 (Index 336) (SNMP ifIndex 16)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Default Is-Primary
        Local: 10.10.0.1
    Protocol iso, MTU: Unlimited
      Addresses, Flags: Is-Default Is-Primary
        Local: 49.0001.0100.1000.0001

  Logical interface lo0.16384 (Index 324) (SNMP ifIndex 21)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 672
    Output packets: 672
    Protocol inet, MTU: Unlimited
      Addresses
        Local: 127.0.0.1

  Logical interface lo0.16385 (Index 325) (SNMP ifIndex 22)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 3375
    Output packets: 3375
    Protocol inet, MTU: Unlimited
      Addresses, Flags: Is-Default Is-Primary
        Local: 128.0.0.1
      Addresses
        Local: 128.0.0.4
    Protocol inet6, MTU: Unlimited
        Local: fe80::207:f:fc00:15

  Logical interface lo0.32768 (Index 320) (SNMP ifIndex 250)
    Flags: Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0

Physical interface: lsi, Enabled, Physical link is Up
  Interface index: 4, SNMP ifIndex: 4
  Type: Software-Pseudo, Link-level type: LSI, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: mtun, Enabled, Physical link is Up
  Interface index: 64, SNMP ifIndex: 12
  Type: Multicast-GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: pimd, Enabled, Physical link is Up
  Interface index: 26, SNMP ifIndex: 11
  Type: PIMD, Link-level type: PIM-Decapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pime, Enabled, Physical link is Up
  Interface index: 25, SNMP ifIndex: 10
  Type: PIME, Link-level type: PIM-Encapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pip0, Enabled, Physical link is Up
  Interface index: 132, SNMP ifIndex: 504
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:42:b0, Hardware address: 00:05:86:71:42:b0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: pp0, Enabled, Physical link is Up
  Interface index: 133, SNMP ifIndex: 505
  Type: PPPoE, Link-level type: PPPoE, MTU: 1532
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None

Physical interface: tap, Enabled, Physical link is Up
  Interface index: 12, SNMP ifIndex: 7
  Type: Software-Pseudo, Link-level type: Interface-Specific, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: vtep, Enabled, Physical link is Up
  Interface index: 135, SNMP ifIndex: 506
  Type: Software-Pseudo, Link-level type: VxLAN-Tunnel-Endpoint, MTU: 1600, Speed: Unlimited
  Device flags   : Present Running
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

