show lldp neighbors | no-more
Local Interface    Parent Interface    Chassis Id          Port info          System Name
ge-0/0/11          -                   00:01:00:6b:ea:12   Ethernet3          sjc-dc12-dist07     
ge-0/0/10          -                   00:02:00:b5:8b:76   Ethernet3          sjc-dc12-dist08     
ge-0/0/9           -                   00:03:00:2a:be:fd   Ethernet3          sjc-dc12-dist09     
ge-0/0/8           -                   00:04:00:f2:76:00   Ethernet3          sjc-dc12-dist10     
ge-0/0/4           -                   00:05:86:71:0c:c0   ge-0/0/3           sjc-core-pe02       
ge-0/0/6           ae1                 00:05:86:71:57:c0   ge-0/0/2           sjc-isp-edge02      
ge-0/0/19          ae1                 00:05:86:71:57:c0   ge-0/0/3           sjc-isp-edge02      
ge-0/0/3           -                   00:05:86:71:7c:c0   ge-0/0/3           sjc-core-pe01       
ge-0/0/7           -                   00:05:86:71:9e:c0   ge-0/0/7           sjc-ce02            
ge-0/0/5           ae0                 00:05:86:71:e9:c0   ge-0/0/2           sjc-isp-edge01      
ge-0/0/18          ae0                 00:05:86:71:e9:c0   ge-0/0/3           sjc-isp-edge01      
ge-0/0/2           -                   00:08:00:00:00:3b   ethernet1/1        PA-VM               
ge-0/0/15          -                   00:18:00:79:64:89   Ethernet3          sjc-dc12-dist03     
ge-0/0/14          -                   00:19:00:89:ce:11   Ethernet3          sjc-dc12-dist04     


LLDP nbr -- interface ge-0/0/11
LLDP Neighbor Information:
Local Information:
Index: 8 Time to live: 120 Time mark: Thu Aug 31 22:55:52 2017 Age: 12 secs 
Local Interface    : ge-0/0/11
Parent Interface   : -
Local Port ID      : 527
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:01:00:6b:ea:12
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist07
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.107
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3




LLDP nbr -- interface ge-0/0/10
LLDP Neighbor Information:
Local Information:
Index: 17 Time to live: 120 Time mark: Thu Aug 31 22:55:53 2017 Age: 11 secs 
Local Interface    : ge-0/0/10
Parent Interface   : -
Local Port ID      : 526
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:02:00:b5:8b:76
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist08
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.108
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3




LLDP nbr -- interface ge-0/0/9
LLDP Neighbor Information:
Local Information:
Index: 15 Time to live: 120 Time mark: Thu Aug 31 22:55:41 2017 Age: 23 secs 
Local Interface    : ge-0/0/9
Parent Interface   : -
Local Port ID      : 522
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:03:00:2a:be:fd
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist09
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.109
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3




LLDP nbr -- interface ge-0/0/8
LLDP Neighbor Information:
Local Information:
Index: 16 Time to live: 120 Time mark: Thu Aug 31 22:55:48 2017 Age: 16 secs 
Local Interface    : ge-0/0/8
Parent Interface   : -
Local Port ID      : 521
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:04:00:f2:76:00
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist10
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.110
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3




LLDP nbr -- interface ge-0/0/4
LLDP Neighbor Information:
Local Information:
Index: 3 Time to live: 40 Time mark: Thu Aug 31 22:56:02 2017 Age: 2 secs 
Local Interface    : ge-0/0/4
Parent Interface   : -
Local Port ID      : 517
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:0c:c0
Port type          : Interface name
Port ID            : ge-0/0/3
Port description   : To SJC-CE01
System name        : sjc-core-pe02
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1518)
       Index    : 3

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (103), VLAN Name (vlan-103)
       Index    : 4

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (105), VLAN Name (vlan-105)
       Index    : 5

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (107), VLAN Name (vlan-107)
       Index    : 6

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (108), VLAN Name (vlan-108)
       Index    : 7




LLDP nbr -- interface ge-0/0/6
LLDP Neighbor Information:
Local Information:
Index: 4 Time to live: 40 Time mark: Thu Aug 31 22:55:58 2017 Age: 6 secs 
Local Interface    : ge-0/0/6
Parent Interface   : ae1
Local Port ID      : 519
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:57:c0
Port type          : Interface name
Port ID            : ge-0/0/2
Port description   : ge-0/0/2
System name        : sjc-isp-edge02
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (524)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/19
LLDP Neighbor Information:
Local Information:
Index: 1 Time to live: 40 Time mark: Thu Aug 31 22:55:59 2017 Age: 5 secs 
Local Interface    : ge-0/0/19
Parent Interface   : ae1
Local Port ID      : 535
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:57:c0
Port type          : Interface name
Port ID            : ge-0/0/3
Port description   : ge-0/0/3
System name        : sjc-isp-edge02
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (524)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/3
LLDP Neighbor Information:
Local Information:
Index: 19 Time to live: 40 Time mark: Thu Aug 31 22:55:59 2017 Age: 5 secs 
Local Interface    : ge-0/0/3
Parent Interface   : -
Local Port ID      : 516
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:7c:c0
Port type          : Interface name
Port ID            : ge-0/0/3
Port description   : To SJC-CE01
System name        : sjc-core-pe01
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1518)
       Index    : 3

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (103), VLAN Name (vlan-103)
       Index    : 4

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (105), VLAN Name (vlan-105)
       Index    : 5

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (107), VLAN Name (vlan-107)
       Index    : 6

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : VLAN Name (3)
       Info     : VLAN ID (108), VLAN Name (vlan-108)
       Index    : 7




LLDP nbr -- interface ge-0/0/7
LLDP Neighbor Information:
Local Information:
Index: 2 Time to live: 40 Time mark: Thu Aug 31 22:56:04 2017 Age: 0 secs 
Local Interface    : ge-0/0/7
Parent Interface   : -
Local Port ID      : 520
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:9e:c0
Port type          : Interface name
Port ID            : ge-0/0/7
Port description   : ge-0/0/7
System name        : sjc-ce02
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/5
LLDP Neighbor Information:
Local Information:
Index: 7 Time to live: 40 Time mark: Thu Aug 31 22:55:59 2017 Age: 6 secs 
Local Interface    : ge-0/0/5
Parent Interface   : ae0
Local Port ID      : 518
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:e9:c0
Port type          : Interface name
Port ID            : ge-0/0/2
Port description   : ge-0/0/2
System name        : sjc-isp-edge01
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (523)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/18
LLDP Neighbor Information:
Local Information:
Index: 6 Time to live: 40 Time mark: Thu Aug 31 22:55:58 2017 Age: 7 secs 
Local Interface    : ge-0/0/18
Parent Interface   : ae0
Local Port ID      : 534
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:e9:c0
Port type          : Interface name
Port ID            : ge-0/0/3
Port description   : ge-0/0/3
System name        : sjc-isp-edge01
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (523)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/2
LLDP Neighbor Information:
Local Information:
Index: 18 Time to live: 121 Time mark: Thu Aug 31 22:55:44 2017 Age: 21 secs 
Local Interface    : ge-0/0/2
Parent Interface   : -
Local Port ID      : 515
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:08:00:00:00:3b
Port type          : Interface name
Port ID            : ethernet1/1
System name        : PA-VM
  
System Description : Palo Alto Networks VM-Series firewall


System capabilities 
        Supported: Other Repeater Bridge Router 
        Enabled  : Other Router 

Management address 
        Address Type      : 802 MAC(6)
        Address           : 00:08:00:00:00:3b
        Interface Number  : 16
        Interface Subtype : ifIndex(2)
        OID               : 43.6.1.4.1.129.198.117.2.3.29.







LLDP nbr -- interface ge-0/0/15
LLDP Neighbor Information:
Local Information:
Index: 12 Time to live: 120 Time mark: Thu Aug 31 22:56:00 2017 Age: 5 secs 
Local Interface    : ge-0/0/15
Parent Interface   : -
Local Port ID      : 531
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:18:00:79:64:89
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist03
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.103
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3




LLDP nbr -- interface ge-0/0/14
LLDP Neighbor Information:
Local Information:
Index: 11 Time to live: 120 Time mark: Thu Aug 31 22:55:40 2017 Age: 25 secs 
Local Interface    : ge-0/0/14
Parent Interface   : -
Local Port ID      : 530
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:19:00:89:ce:11
Port type          : Interface name
Port ID            : Ethernet3
System name        : sjc-dc12-dist04
  
System Description : Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Management address 
        Address Type      : IPv4(1)
        Address           : 10.117.255.104
        Interface Number  : 5000000
        Interface Subtype : ifIndex(2)

Organization Info
       OUI      : Ethernet Bridged (0x0080c2)
       Subtype  : (1)
       Info     : 0000 
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (9236)
       Index    : 3






