Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  Internet address is 10.100.0.76/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     27776 packets input, 2489344 bytes
     Received 1 broadcasts, 52 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     95395 packets output, 19127676 bytes
     Sent 3 broadcasts, 40106 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     43 packets input, 2752 bytes
     Received 0 broadcasts, 43 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40110 packets output, 7258730 bytes
     Sent 0 broadcasts, 40110 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.0013 (bia 0020.0000.0013)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     10142661 packets input, 842841364 bytes
     Received 801952 broadcasts, 9340596 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     43212 packets output, 7595977 bytes
     Sent 83 broadcasts, 43129 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.0017 (bia 0020.0000.0017)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     10173573 packets input, 845035860 bytes
     Received 801926 broadcasts, 9371448 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     43405 packets output, 7619284 bytes
     Sent 91 broadcasts, 43309 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.001b (bia 0020.0000.001b)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     42 packets input, 2688 bytes
     Received 0 broadcasts, 42 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10181183 packets output, 841944704 bytes
     Sent 802010 broadcasts, 9379059 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.0020 (bia 0020.0000.0020)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     42 packets input, 2688 bytes
     Received 0 broadcasts, 42 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10181176 packets output, 841944204 bytes
     Sent 802010 broadcasts, 9379052 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.0025 (bia 0020.0000.0025)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     42 packets input, 2688 bytes
     Received 0 broadcasts, 42 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10181175 packets output, 841944023 bytes
     Sent 802010 broadcasts, 9379051 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:06:31 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     42 packets input, 2688 bytes
     Received 0 broadcasts, 42 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40108 packets output, 7258555 bytes
     Sent 0 broadcasts, 40108 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41 packets input, 2624 bytes
     Received 0 broadcasts, 41 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40108 packets output, 7258649 bytes
     Sent 0 broadcasts, 40108 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     39 packets input, 2496 bytes
     Received 0 broadcasts, 39 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40106 packets output, 7298699 bytes
     Sent 0 broadcasts, 40106 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.009c.da72
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 56 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40 packets input, 2560 bytes
     Received 0 broadcasts, 40 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40107 packets output, 7298755 bytes
     Sent 0 broadcasts, 40107 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.117.255.12/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 51 minutes, 9 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0020.0000.0007 (bia 0020.0000.0007)
  Internet address is 10.117.38.22/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 1 minutes, 51 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40109 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
