edge-7
host-85

VDR edge-7 LIF Information :

Name:                c3500000000b
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50002
Ip(Mask):            192.168.73.1(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c3500000000a
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50001
Ip(Mask):            192.168.72.1(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c35000000002
Mode:                Routing, Distributed, Uplink
Id:                  Vxlan:50000
Ip(Mask):            192.168.102.50(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2208
DHCP Relay:          Not enabled



---

edge-7
host-51

VDR edge-7 LIF Information :

Name:                c3500000000b
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50002
Ip(Mask):            192.168.73.1(255.255.255.0)
Connected Dvs:       atl-nsx-Dswitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c3500000000a
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50001
Ip(Mask):            192.168.72.1(255.255.255.0)
Connected Dvs:       atl-nsx-Dswitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c35000000002
Mode:                Routing, Distributed, Uplink
Id:                  Vxlan:50000
Ip(Mask):            192.168.102.50(255.255.255.0)
Connected Dvs:       atl-nsx-Dswitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2208
DHCP Relay:          Not enabled



---

edge-7
host-77

VDR edge-7 LIF Information :

Name:                c3500000000b
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50002
Ip(Mask):            192.168.73.1(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c3500000000a
Mode:                Routing, Distributed, Internal
Id:                  Vxlan:50001
Ip(Mask):            192.168.72.1(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2288
DHCP Relay:          Not enabled

Name:                c35000000002
Mode:                Routing, Distributed, Uplink
Id:                  Vxlan:50000
Ip(Mask):            192.168.102.50(255.255.255.0)
Connected Dvs:       sjc-nsx-DSwitch 
VXLAN Control Plane: Enabled 
VXLAN Multicast IP:  0.0.0.1 
State:               Enabled
Flags:               0x2208
DHCP Relay:          Not enabled



---

