! Command: show running-config
! device: atl-dc01-acc12 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname atl-dc01-acc12
!
spanning-tree mode mstp
!
!
no aaa root
!
!
vlan 212,254-255
!
vrf definition CORP-PROD1
   rd 1:104
!
interface Ethernet1
   no switchport
   ip address 10.100.0.184/31
!
interface Ethernet2
   no switchport
!
interface Ethernet2.104
   encapsulation dot1q vlan 104
   vrf forwarding CORP-PROD1
   ip address 10.110.1.93/31
   isis enable Osiris-CORP-PROD1
   isis network point-to-point
!
interface Ethernet3
   no switchport
!
interface Ethernet3.104
   encapsulation dot1q vlan 104
   vrf forwarding CORP-PROD1
   ip address 10.110.1.89/31
   isis enable Osiris-CORP-PROD1
   isis network point-to-point
!
interface Ethernet4
   switchport access vlan 212
!
interface Ethernet5
   switchport access vlan 212
!
interface Ethernet6
   switchport access vlan 212
!
interface Ethernet7
   switchport access vlan 212
!
interface Ethernet8
   no switchport
!
interface Ethernet9
   no switchport
!
interface Ethernet10
   no switchport
!
interface Ethernet11
   no switchport
!
interface Ethernet12
   no switchport
!
interface Ethernet13
   no switchport
!
interface Ethernet14
   no switchport
!
interface Ethernet15
   no switchport
!
interface Ethernet16
   no switchport
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   no switchport
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.110.4.14/32
!
interface Management1
   ip address 10.110.37.22/24
!
interface Vlan212
   vrf forwarding CORP-PROD1
   ip address 10.101.15.129/25
!
ip routing
ip routing vrf CORP-PROD1
!
router isis Osiris-CORP-PROD1 vrf CORP-PROD1
   net 49.0001.0101.1000.4014.00
   is-type level-2
   redistribute connected
   redistribute static
   address-family ipv4 unicast
!
management ssh
   idle-timeout 300
!
!
end
