Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  Internet address is 10.100.0.96/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     29269 packets input, 2595415 bytes
     Received 1 broadcasts, 43 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     98992 packets output, 19656348 bytes
     Sent 3 broadcasts, 40099 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     34 packets input, 2176 bytes
     Received 0 broadcasts, 34 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40103 packets output, 7257521 bytes
     Sent 0 broadcasts, 40103 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.002a (bia 0013.0000.002a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     8834957 packets input, 699254543 bytes
     Received 801677 broadcasts, 8032909 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40186 packets output, 7263544 bytes
     Sent 0 broadcasts, 40186 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.002f (bia 0013.0000.002f)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     8861874 packets input, 701241185 bytes
     Received 801670 broadcasts, 8059736 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40394 packets output, 7278417 bytes
     Sent 22 broadcasts, 40372 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.0033 (bia 0013.0000.0033)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     33 packets input, 2112 bytes
     Received 0 broadcasts, 33 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8861418 packets output, 698010239 bytes
     Sent 801656 broadcasts, 8059391 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.0037 (bia 0013.0000.0037)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     34 packets input, 2176 bytes
     Received 0 broadcasts, 34 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8861420 packets output, 698010476 bytes
     Sent 801656 broadcasts, 8059393 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.003b (bia 0013.0000.003b)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     34 packets input, 2176 bytes
     Received 0 broadcasts, 34 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8861419 packets output, 698010264 bytes
     Sent 801656 broadcasts, 8059392 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:03:56 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     36 packets input, 2304 bytes
     Received 0 broadcasts, 36 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40105 packets output, 7257695 bytes
     Sent 0 broadcasts, 40105 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     36 packets input, 2304 bytes
     Received 0 broadcasts, 36 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40104 packets output, 7257639 bytes
     Sent 0 broadcasts, 40104 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     31 packets input, 1984 bytes
     Received 0 broadcasts, 31 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40099 packets output, 7297484 bytes
     Sent 0 broadcasts, 40099 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.00bc.e2a7
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 3 minutes, 17 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     32 packets input, 2048 bytes
     Received 0 broadcasts, 32 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40100 packets output, 7297540 bytes
     Sent 0 broadcasts, 40100 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.117.255.42/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 51 minutes, 53 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0013.0000.001e (bia 0013.0000.001e)
  Internet address is 10.117.38.36/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 2 minutes, 28 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40102 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
