Displaying 3 of 3 IPv6 routing table entries
Codes: C - connected, S - static, K - kernel, O - OSPF, B - BGP, R - RIP, A B - BGP Aggregate, A O - OSPF Summary, I - ISIS

 K    ::1/128 [1/0]
       directly connected, <Internal>
 K    ::/96 [1/0]
       directly connected, <Internal>
 C    fe80::/10 [1/0]
       directly connected, <Internal>

! IPv6 routing not enabled
