! Command: show running-config
! device: atl-dc01-acc01 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname atl-dc01-acc01
!
spanning-tree mode mstp
!
!
no aaa root
!
!
vlan 201
!
vrf definition ECOMM-1-PROD
   rd 1:101
!
interface Ethernet1
   no switchport
   ip address 10.100.0.216/31
!
interface Ethernet2
   no switchport
!
interface Ethernet2.101
   encapsulation dot1q vlan 101
   vrf forwarding ECOMM-1-PROD
   ip address 10.110.1.5/31
   isis enable Osiris-ECOMM-1-PROD
   isis network point-to-point
!
interface Ethernet3
   no switchport
!
interface Ethernet3.101
   encapsulation dot1q vlan 101
   vrf forwarding ECOMM-1-PROD
   ip address 10.110.1.1/31
   isis enable Osiris-ECOMM-1-PROD
   isis network point-to-point
!
interface Ethernet4
   switchport access vlan 201
!
interface Ethernet5
   switchport access vlan 201
!
interface Ethernet6
   switchport access vlan 201
!
interface Ethernet7
   switchport access vlan 201
!
interface Ethernet8
   no switchport
!
interface Ethernet9
   no switchport
!
interface Ethernet10
   no switchport
!
interface Ethernet11
   no switchport
!
interface Ethernet12
   no switchport
!
interface Ethernet13
   no switchport
!
interface Ethernet14
   no switchport
!
interface Ethernet15
   no switchport
!
interface Ethernet16
   no switchport
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   no switchport
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.10.4.3/32
!
interface Management1
   ip address 10.110.37.11/24
!
interface Vlan201
   vrf forwarding ECOMM-1-PROD
   ip address 10.101.10.1/25
!
ip routing
ip routing vrf ECOMM-1-PROD
!
router isis Osiris-ECOMM-1-PROD vrf ECOMM-1-PROD
   net 49.0001.0101.1000.4003.00
   is-type level-2
   redistribute connected
   redistribute static
   address-family ipv4 unicast
!
management ssh
   idle-timeout 300
!
!
end
