## Last commit: 2017-08-25 07:27:16 UTC by testuser
version 14.1R5.4;
system {
    host-name usa-core-p02;
    default-address-selection;
    services {
        ssh {
            protocol-version v2;
        }
    }
    syslog {
        file messages {
            any notice;
            authorization info;
        }
        file interactive-commands {
            interactive-commands any;
        }
    }
}
chassis {
    aggregated-devices {
        ethernet {
            device-count 2;
        }
    }
    fpc 0 {
        pic 0 {
            number-of-ports 23;
        }
    }
}
interfaces {
    ge-0/0/0 {
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.100.0.50/31;
            }
            family iso;
        }
    }
    ge-0/0/1 {
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.22/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/2 {
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.30/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/3 {
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.6/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/4 {
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.14/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/5 {
        disable;
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.38/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/6 {
        disable;
        link-mode full-duplex;
        unit 0 {
            family inet {
                address 10.10.1.46/30;
            }
            family iso;
            family mpls;
        }
    }
    ge-0/0/7 {
        link-mode full-duplex;
    }
    lo0 {
        unit 0 {
            family inet {
                address 10.10.0.2/32;
            }
            family iso {
                address 49.0001.0100.1000.0002.00;
            }
        }
    }
}
routing-options {
    router-id 10.10.0.2;
    autonomous-system 10;
    forwarding-table {
        export LOAD_BALANCE;
    }
}
protocols {
    mpls {
        interface ge-0/0/1.0;
        interface ge-0/0/2.0;
        interface ge-0/0/3.0;
        interface ge-0/0/4.0;
        interface ge-0/0/5.0;
        interface ge-0/0/6.0;
    }
    isis {
        level 2 wide-metrics-only;
        interface ge-0/0/1.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface ge-0/0/2.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface ge-0/0/3.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface ge-0/0/4.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface ge-0/0/5.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface ge-0/0/6.0 {
            level 2 metric 10000;
            level 1 disable;
        }
        interface lo0.0;
    }
    ldp {
        interface ge-0/0/1.0;
        interface ge-0/0/2.0;
        interface ge-0/0/3.0;
        interface ge-0/0/4.0;
        interface ge-0/0/5.0;
        interface ge-0/0/6.0;
    }
    lldp {
        interface all;
    }
}
policy-options {
    policy-statement LOAD_BALANCE {
        then {
            load-balance per-packet;
        }
    }
    policy-statement export-direct {
        term from-direct {
            from protocol direct;
            then accept;
        }
    }
    policy-statement export-statics {
        term from-static {
            from protocol static;
            then accept;
        }
    }
}
firewall {
    family inet {
        filter man-filter {
            term 1 {
                from {
                    source-address {
                        0.0.0.0/0;
                    }
                    destination-address {
                        10.100.0.18/32;
                        10.100.0.16/32;
                    }
                }
                then accept;
            }
        }
    }
}
