! Command: show running-config
! device: sjc-dc12-dist09 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-dist09
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1201-1210 priority 4096
!
!
no aaa root
!
!
vlan 1201-1210
!
vrf definition MGT-TOOLS
   rd 2:105
!
interface Ethernet1
   no switchport
   ip address 10.100.0.30/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   no switchport
   vrf forwarding MGT-TOOLS
   ip address 10.115.5.34/31
!
interface Ethernet4
   no switchport
   vrf forwarding MGT-TOOLS
   ip address 10.115.5.36/31
!
interface Ethernet5
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet6
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet7
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet8
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet9
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet10
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet11
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet12
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet13
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet14
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet15
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet16
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   switchport trunk allowed vlan 1201-1210
   switchport mode trunk
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.117.255.109/32
!
interface Management1
   ip address 10.117.38.79/24
!
interface Vlan1201
   vrf forwarding MGT-TOOLS
   ip address 10.117.201.2/24
   ip virtual-router address 10.117.201.1
!
interface Vlan1202
   vrf forwarding MGT-TOOLS
   ip address 10.117.202.2/24
   ip virtual-router address 10.117.202.1
!
interface Vlan1203
   vrf forwarding MGT-TOOLS
   ip address 10.117.203.2/24
   ip virtual-router address 10.117.203.1
!
interface Vlan1204
   vrf forwarding MGT-TOOLS
   ip address 10.117.204.2/24
   ip virtual-router address 10.117.204.1
!
interface Vlan1205
   vrf forwarding MGT-TOOLS
   ip address 10.117.205.2/24
   ip virtual-router address 10.117.205.1
!
interface Vlan1206
   vrf forwarding MGT-TOOLS
   ip address 10.117.206.2/24
   ip virtual-router address 10.117.206.1
!
interface Vlan1207
   vrf forwarding MGT-TOOLS
   ip address 10.117.207.2/24
   ip virtual-router address 10.117.207.1
!
interface Vlan1208
   vrf forwarding MGT-TOOLS
   ip address 10.117.208.2/24
   ip virtual-router address 10.117.208.1
!
interface Vlan1209
   vrf forwarding MGT-TOOLS
   ip address 10.117.209.2/24
   ip virtual-router address 10.117.209.1
!
interface Vlan1210
   vrf forwarding MGT-TOOLS
   ip address 10.117.210.2/24
   ip virtual-router address 10.117.210.1
!
ip virtual-router mac-address 00:1c:73:00:00:05
!
ip routing
ip routing vrf MGT-TOOLS
!
route-map TAG-OSPF permit 10
   set tag 100105
!
router ospf 1 vrf MGT-TOOLS
   router-id 10.117.255.109
   redistribute connected route-map TAG-OSPF
   network 10.115.5.34/31 area 0.0.0.0
   network 10.115.5.36/31 area 0.0.0.0
   network 10.117.202.0/24 area 0.0.0.0
   max-lsa 12000
!
!
end
