Interface Ethernet1 detected 0 LLDP neighbors:

Interface Ethernet2 detected 0 LLDP neighbors:

Interface Ethernet3 detected 1 LLDP neighbors:

  Neighbor 0005.8671.f0c0/ge-0/0/9, age 9 seconds
  Discovered 23:55:52 ago; Last changed 23:55:52 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.f0c0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/9"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/9"
    - System Name: "sjc-ce01"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet4 detected 1 LLDP neighbors:

  Neighbor 0005.8671.9ec0/ge-0/0/9, age 0 seconds
  Discovered 23:55:46 ago; Last changed 23:55:46 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.9ec0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/9"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/9"
    - System Name: "sjc-ce02"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet5 detected 1 LLDP neighbors:

  Neighbor 0015.0066.a9d7/Ethernet3, age 8 seconds
  Discovered 23:55:41 ago; Last changed 23:55:41 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0015.0066.a9d7
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc401"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.81
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet6 detected 1 LLDP neighbors:

  Neighbor 0016.00ef.7373/Ethernet3, age 6 seconds
  Discovered 23:55:41 ago; Last changed 23:55:41 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0016.00ef.7373
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc402"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.82
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet7 detected 1 LLDP neighbors:

  Neighbor 0017.00a4.ca3f/Ethernet3, age 23 seconds
  Discovered 23:55:28 ago; Last changed 23:55:28 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0017.00a4.ca3f
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc403"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.83
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet8 detected 1 LLDP neighbors:

  Neighbor 0018.00c8.a17d/Ethernet3, age 28 seconds
  Discovered 23:55:31 ago; Last changed 23:55:31 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0018.00c8.a17d
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc404"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.84
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet9 detected 1 LLDP neighbors:

  Neighbor 0019.00f8.5996/Ethernet3, age 1 seconds
  Discovered 23:55:28 ago; Last changed 23:55:28 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0019.00f8.5996
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc405"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.85
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet10 detected 1 LLDP neighbors:

  Neighbor 0020.008e.b269/Ethernet3, age 10 seconds
  Discovered 23:55:37 ago; Last changed 23:55:37 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0020.008e.b269
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc406"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.86
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet11 detected 1 LLDP neighbors:

  Neighbor 0021.0002.acc2/Ethernet3, age 18 seconds
  Discovered 23:55:47 ago; Last changed 23:55:47 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0021.0002.acc2
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc407"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.87
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet12 detected 1 LLDP neighbors:

  Neighbor 0001.00cf.d8c8/Ethernet3, age 16 seconds
  Discovered 23:55:37 ago; Last changed 23:55:37 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0001.00cf.d8c8
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc408"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.88
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet13 detected 1 LLDP neighbors:

  Neighbor 0002.003e.1433/Ethernet3, age 25 seconds
  Discovered 23:55:26 ago; Last changed 23:55:26 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0002.003e.1433
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc409"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.89
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet14 detected 1 LLDP neighbors:

  Neighbor 0003.0051.b6e0/Ethernet3, age 4 seconds
  Discovered 23:55:33 ago; Last changed 23:55:33 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0003.0051.b6e0
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc410"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.90
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet15 detected 1 LLDP neighbors:

  Neighbor 0004.00d6.4453/Ethernet3, age 16 seconds
  Discovered 23:55:37 ago; Last changed 23:55:37 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0004.00d6.4453
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc411"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.91
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet16 detected 1 LLDP neighbors:

  Neighbor 0005.0068.2a52/Ethernet3, age 20 seconds
  Discovered 23:55:26 ago; Last changed 23:55:26 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.0068.2a52
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc412"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.92
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet17 detected 0 LLDP neighbors:

Interface Ethernet18 detected 1 LLDP neighbors:

  Neighbor 0004.00f2.7600/Ethernet18, age 12 seconds
  Discovered 23:55:41 ago; Last changed 23:55:41 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0004.00f2.7600
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet18"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-dist10"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.110
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet19 detected 0 LLDP neighbors:

Interface Management1 detected 0 LLDP neighbors:

