
MAC flags (S - static MAC, D - dynamic MAC, L - locally learned, P - Persistent static, C - Control MAC
           SE - statistics enabled, NM - non configured MAC, R - remote PE MAC, O - ovsdb MAC)


Ethernet switching table : 5 entries, 5 learned
Routing instance : default-switch
    Vlan                MAC                 MAC         Age    Logical                NH        RTR 
    name                address             flags              interface              Index     ID
    vl1170              00:0c:29:90:1f:57   D             -   ge-1/0/1.0             0         0       
    vl1170              00:50:56:68:e7:aa   D             -   ge-1/0/1.0             0         0       
    vl1170              00:50:56:6c:d3:89   D             -   ge-1/0/0.0             0         0       
    vl214               00:50:56:65:60:1a   D             -   ge-1/0/1.0             0         0       
    vl30                00:50:56:bd:6b:2b   D             -   ge-1/0/0.0             0         0       

