Physical interface: ge-0/0/0, Enabled, Physical link is Up
  Interface index: 139, SNMP ifIndex: 513
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:04, Hardware address: 00:12:00:00:00:04
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 984 bps (0 pps)
  Output rate    : 144 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/0.0 (Index 329) (SNMP ifIndex 525)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 96859
    Output packets: 306279
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.100.0.130/31, Local: 10.100.0.130
    Protocol iso, MTU: 1497
      Flags: Is-Primary
    Protocol multiservice, MTU: Unlimited
      Flags: Is-Primary

Physical interface: lc-0/0/0, Enabled, Physical link is Up
  Interface index: 136, SNMP ifIndex: 507
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-0/0/0.32769 (Index 326) (SNMP ifIndex 508)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited
      Flags: Is-Primary

Physical interface: pfe-0/0/0, Enabled, Physical link is Up
  Interface index: 138, SNMP ifIndex: 511
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-0/0/0.16383 (Index 328) (SNMP ifIndex 512)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
      Flags: None

Physical interface: pfh-0/0/0, Enabled, Physical link is Up
  Interface index: 137, SNMP ifIndex: 509
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfh-0/0/0.16383 (Index 327) (SNMP ifIndex 510)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/1, Enabled, Physical link is Up
  Interface index: 140, SNMP ifIndex: 514
  Description: To SJC-APP-LB01
  Link-level type: Ethernet, MTU: 1518, MRU: 1526, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:05, Hardware address: 00:12:00:00:00:05
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 800 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/1.103 (Index 339) (SNMP ifIndex 541)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.103 ]  Encapsulation: ENET2
    Input packets : 44
    Output packets: 137418
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.58/31, Local: 10.115.7.59
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.105 (Index 340) (SNMP ifIndex 542)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.105 ]  Encapsulation: ENET2
    Input packets : 0
    Output packets: 137456
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.62/31, Local: 10.115.7.63
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.108 (Index 341) (SNMP ifIndex 543)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.108 ]  Encapsulation: ENET2
    Input packets : 1259
    Output packets: 138407
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.7.52/31, Local: 10.115.7.52
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.109 (Index 342) (SNMP ifIndex 544)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.109 ]  Encapsulation: ENET2
    Input packets : 1100
    Output packets: 138331
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.54/31, Local: 10.115.7.54
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.110 (Index 343) (SNMP ifIndex 545)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.110 ]  Encapsulation: ENET2
    Input packets : 1167
    Output packets: 138480
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.56/31, Local: 10.115.7.56
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.111 (Index 344) (SNMP ifIndex 546)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.111 ]  Encapsulation: ENET2
    Input packets : 0
    Output packets: 137395
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.60/31, Local: 10.115.7.61
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/1.32767 (Index 345) (SNMP ifIndex 547)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 0
    Output packets: 129733
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/2, Enabled, Physical link is Up
  Interface index: 141, SNMP ifIndex: 515
  Description: To SJC-TE-FW01
  Link-level type: Ethernet, MTU: 1518, MRU: 1526, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:06, Hardware address: 00:12:00:00:00:06
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 496 bps (0 pps)
  Output rate    : 960 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/2.103 (Index 356) (SNMP ifIndex 558)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.103 ]  Encapsulation: ENET2
    Input packets : 161501
    Output packets: 171203
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.32/31, Local: 10.115.7.33
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.105 (Index 357) (SNMP ifIndex 559)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.105 ]  Encapsulation: ENET2
    Input packets : 160380
    Output packets: 172123
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.36/31, Local: 10.115.7.37
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.107 (Index 358) (SNMP ifIndex 560)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.107 ]  Encapsulation: ENET2
    Input packets : 465801
    Output packets: 473174
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.26/31, Local: 10.115.7.27
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.108 (Index 359) (SNMP ifIndex 561)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.108 ]  Encapsulation: ENET2
    Input packets : 654099
    Output packets: 884628
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.24/31, Local: 10.115.7.25
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.109 (Index 360) (SNMP ifIndex 562)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.109 ]  Encapsulation: ENET2
    Input packets : 158618
    Output packets: 170806
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.28/31, Local: 10.115.7.29
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.110 (Index 361) (SNMP ifIndex 563)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.110 ]  Encapsulation: ENET2
    Input packets : 157475
    Output packets: 170486
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.30/31, Local: 10.115.7.31
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.111 (Index 362) (SNMP ifIndex 564)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.111 ]  Encapsulation: ENET2
    Input packets : 157959
    Output packets: 170673
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.34/31, Local: 10.115.7.35
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.208 (Index 379) (SNMP ifIndex 581)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.208 ]  Encapsulation: ENET2
    Input packets : 503862
    Output packets: 862080
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.7.100/31, Local: 10.115.7.100
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/2.32767 (Index 363) (SNMP ifIndex 565)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 39994
    Output packets: 129699
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/3, Enabled, Physical link is Up
  Interface index: 142, SNMP ifIndex: 516
  Description: To SJC-CORE-PE01
  Link-level type: Ethernet, MTU: 1518, MRU: 1526, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:07, Hardware address: 00:12:00:00:00:07
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 304 bps (0 pps)
  Output rate    : 832 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/3.103 (Index 364) (SNMP ifIndex 566)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.103 ]  Encapsulation: ENET2
    Input packets : 88313
    Output packets: 225906
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.4/31, Local: 10.10.1.4
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/3.105 (Index 365) (SNMP ifIndex 567)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.105 ]  Encapsulation: ENET2
    Input packets : 89214
    Output packets: 225937
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.8/31, Local: 10.10.1.8
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/3.107 (Index 366) (SNMP ifIndex 568)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.107 ]  Encapsulation: ENET2
    Input packets : 79771
    Output packets: 219557
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.12/31, Local: 10.10.1.12
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/3.108 (Index 367) (SNMP ifIndex 569)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.108 ]  Encapsulation: ENET2
    Input packets : 87907
    Output packets: 224651
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.10/31, Local: 10.10.1.10
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/3.32767 (Index 368) (SNMP ifIndex 570)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 129581
    Output packets: 129739
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/4, Enabled, Physical link is Up
  Interface index: 143, SNMP ifIndex: 517
  Description: To SJC-CORE-PE02
  Link-level type: Ethernet, MTU: 1518, MRU: 1526, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:08, Hardware address: 00:12:00:00:00:08
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 312 bps (0 pps)
  Output rate    : 728 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/4.103 (Index 369) (SNMP ifIndex 571)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.103 ]  Encapsulation: ENET2
    Input packets : 88277
    Output packets: 225763
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.20/31, Local: 10.10.1.20
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/4.105 (Index 370) (SNMP ifIndex 572)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.105 ]  Encapsulation: ENET2
    Input packets : 88361
    Output packets: 225722
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.24/31, Local: 10.10.1.24
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/4.107 (Index 371) (SNMP ifIndex 573)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.107 ]  Encapsulation: ENET2
    Input packets : 79741
    Output packets: 219460
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.28/31, Local: 10.10.1.28
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/4.108 (Index 372) (SNMP ifIndex 574)
    Flags: Up SNMP-Traps 0x4000 VLAN-Tag [ 0x8100.108 ]  Encapsulation: ENET2
    Input packets : 87591
    Output packets: 224342
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.26/31, Local: 10.10.1.26
    Protocol multiservice, MTU: Unlimited

  Logical interface ge-0/0/4.32767 (Index 373) (SNMP ifIndex 575)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 129705
    Output packets: 129717
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/5, Enabled, Physical link is Up
  Interface index: 144, SNMP ifIndex: 518
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:f0:c0, Hardware address: 00:12:00:00:00:09
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 144 bps (0 pps)
  Output rate    : 216 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/5.0 (Index 374) (SNMP ifIndex 576)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 210658
    Output packets: 142290
    Protocol aenet, AE bundle: ae0.0

Physical interface: ge-0/0/6, Enabled, Physical link is Up
  Interface index: 145, SNMP ifIndex: 519
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:f0:c1, Hardware address: 00:12:00:00:00:0a
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 144 bps (0 pps)
  Output rate    : 216 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/6.0 (Index 375) (SNMP ifIndex 577)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 212002
    Output packets: 129712
    Protocol aenet, AE bundle: ae1.0

Physical interface: ge-0/0/7, Enabled, Physical link is Up
  Interface index: 146, SNMP ifIndex: 520
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:0b, Hardware address: 00:12:00:00:00:0b
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 384 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/7.0 (Index 376) (SNMP ifIndex 578)
    Description: To SJC-CE02
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 390746
    Output packets: 437010
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.42/31, Local: 10.115.5.42
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/8, Enabled, Physical link is Up
  Interface index: 147, SNMP ifIndex: 521
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:0c, Hardware address: 00:12:00:00:00:0c
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 136 bps (0 pps)
  Output rate    : 320 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/8.0 (Index 377) (SNMP ifIndex 579)
    Description: To SJC-DC12-DIST10
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 207725
    Output packets: 300457
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.5.38/31, Local: 10.115.5.39
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/9, Enabled, Physical link is Up
  Interface index: 148, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:0d, Hardware address: 00:12:00:00:00:0d
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/9.0 (Index 378) (SNMP ifIndex 580)
    Description: To SJC-DC12-DIST09
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 206781
    Output packets: 302001
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.34/31, Local: 10.115.5.35
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/10, Enabled, Physical link is Up
  Interface index: 149, SNMP ifIndex: 526
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:0e, Hardware address: 00:12:00:00:00:0e
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 264 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/10.0 (Index 346) (SNMP ifIndex 548)
    Description: To SJC-DC12-DIST08
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 209063
    Output packets: 299303
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.5.24/31, Local: 10.115.5.25
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/11, Enabled, Physical link is Up
  Interface index: 150, SNMP ifIndex: 527
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:0f, Hardware address: 00:12:00:00:00:0f
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 256 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/11.0 (Index 347) (SNMP ifIndex 549)
    Description: To SJC-DC12-DIST07
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 208742
    Output packets: 299429
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.22/31, Local: 10.115.5.23
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/12, Enabled, Physical link is Up
  Interface index: 151, SNMP ifIndex: 528
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:10, Hardware address: 00:12:00:00:00:10
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/12.0 (Index 348) (SNMP ifIndex 550)
    Description: To SJC-DC12-DIST06
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 206951
    Output packets: 300062
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.5.16/31, Local: 10.115.5.17
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/13, Enabled, Physical link is Up
  Interface index: 152, SNMP ifIndex: 529
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:11, Hardware address: 00:12:00:00:00:11
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/13.0 (Index 349) (SNMP ifIndex 551)
    Description: To SJC-DC12-DIST05
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 208454
    Output packets: 302220
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.14/31, Local: 10.115.5.15
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/14, Enabled, Physical link is Up
  Interface index: 153, SNMP ifIndex: 530
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:12, Hardware address: 00:12:00:00:00:12
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 120 bps (0 pps)
  Output rate    : 344 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/14.0 (Index 350) (SNMP ifIndex 552)
    Description: To SJC-DC12-DIST04
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 207087
    Output packets: 299565
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.5.12/31, Local: 10.115.5.13
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/15, Enabled, Physical link is Up
  Interface index: 154, SNMP ifIndex: 531
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:13, Hardware address: 00:12:00:00:00:13
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 48 bps (0 pps)
  Output rate    : 296 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/15.0 (Index 351) (SNMP ifIndex 553)
    Description: To SJC-DC12-DIST03
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 208356
    Output packets: 300621
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.10/31, Local: 10.115.5.11
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/16, Enabled, Physical link is Up
  Interface index: 155, SNMP ifIndex: 532
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:14, Hardware address: 00:12:00:00:00:14
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 48 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/16.0 (Index 352) (SNMP ifIndex 554)
    Description: To SJC-DC12-DIST02
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 209616
    Output packets: 299591
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.5.6/31, Local: 10.115.5.7
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/17, Enabled, Physical link is Up
  Interface index: 156, SNMP ifIndex: 533
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:15, Hardware address: 00:12:00:00:00:15
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 48 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/17.0 (Index 353) (SNMP ifIndex 555)
    Description: To SJC-DC12-DIST01
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 209309
    Output packets: 299314
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.5.2/31, Local: 10.115.5.3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/18, Enabled, Physical link is Up
  Interface index: 157, SNMP ifIndex: 534
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:f0:c0, Hardware address: 00:12:00:00:00:16
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 144 bps (0 pps)
  Output rate    : 512 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/18.0 (Index 354) (SNMP ifIndex 556)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 129713
    Output packets: 363620
    Protocol aenet, AE bundle: ae0.0

Physical interface: ge-0/0/19, Enabled, Physical link is Up
  Interface index: 158, SNMP ifIndex: 535
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:f0:c1, Hardware address: 00:12:00:00:00:17
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 144 bps (0 pps)
  Output rate    : 224 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/19.0 (Index 355) (SNMP ifIndex 557)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 129738
    Output packets: 325598
    Protocol aenet, AE bundle: ae1.0

Physical interface: ge-0/0/20, Enabled, Physical link is Up
  Interface index: 159, SNMP ifIndex: 536
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:18, Hardware address: 00:12:00:00:00:18
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/21, Enabled, Physical link is Up
  Interface index: 160, SNMP ifIndex: 537
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:12:00:00:00:19, Hardware address: 00:12:00:00:00:19
  Last flapped   : 2017-08-18 00:53:10 UTC (1w6d 22:02 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/22, Enabled, Physical link is Down
  Interface index: 161, SNMP ifIndex: 538
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:ed:16, Hardware address: 00:05:86:71:ed:16
  Last flapped   : 2017-08-18 00:53:11 UTC (1w6d 22:02 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ae0, Enabled, Physical link is Up
  Interface index: 128, SNMP ifIndex: 523
  Description: To SJC-ISP-EDGE01
  Link-level type: Ethernet, MTU: 1514, Speed: 2Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:f0:c0, Hardware address: 00:05:86:71:f0:c0
  Last flapped   : 2017-08-18 01:06:36 UTC (1w6d 21:49 ago)
  Input rate     : 288 bps (0 pps)
  Output rate    : 736 bps (0 pps)

  Logical interface ae0.0 (Index 337) (SNMP ifIndex 539)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :         80922          0       4999684            0
        Output:        246470          0      19671809          176
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: 10.115.6.10/31, Local: 10.115.6.10
    Protocol multiservice, MTU: Unlimited

Physical interface: ae1, Enabled, Physical link is Up
  Interface index: 129, SNMP ifIndex: 524
  Description: To SJC-ISP-EDGE02
  Link-level type: Ethernet, MTU: 1514, Speed: 2Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:f0:c1, Hardware address: 00:05:86:71:f0:c1
  Last flapped   : 2017-08-18 01:06:36 UTC (1w6d 21:49 ago)
  Input rate     : 288 bps (0 pps)
  Output rate    : 448 bps (0 pps)

  Logical interface ae1.0 (Index 338) (SNMP ifIndex 540)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :         82273          0       4960869            0
        Output:        195864          0      16739035            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.115.6.6/31, Local: 10.115.6.6
    Protocol multiservice, MTU: Unlimited

Physical interface: cbp0, Enabled, Physical link is Up
  Interface index: 131, SNMP ifIndex: 501
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:ed:11, Hardware address: 00:05:86:71:ed:11
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: demux0, Enabled, Physical link is Up
  Interface index: 130, SNMP ifIndex: 502
  Type: Software-Pseudo, MTU: 9192, Clocking: 1
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: dsc, Enabled, Physical link is Up
  Interface index: 5, SNMP ifIndex: 5
  Type: Software-Pseudo, MTU: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: em1, Enabled, Physical link is Up
  Interface index: 9, SNMP ifIndex: 23
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 52:54:00:51:a2:38, Hardware address: 52:54:00:51:a2:38
  Last flapped   : Never
    Input packets : 548589929
    Output packets: 610595961

  Logical interface em1.0 (Index 3) (SNMP ifIndex 24)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 548589929
    Output packets: 610595961
    Protocol inet, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 172.16/16, Local: 172.16.0.1, Broadcast: 172.16.255.255
    Protocol inet6, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred
        Destination: fe80::/64, Local: fe80::5254:ff:fe51:a238

Physical interface: fxp0, Enabled, Physical link is Up
  Interface index: 8, SNMP ifIndex: 1
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Current address: 00:12:00:00:00:1a, Hardware address: 00:12:00:00:00:1a
  Last flapped   : 2017-08-18 00:52:07 UTC (1w6d 22:03 ago)
    Input packets : 20807
    Output packets: 0

Physical interface: gre, Enabled, Physical link is Up
  Interface index: 10, SNMP ifIndex: 8
  Type: GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: ipip, Enabled, Physical link is Up
  Interface index: 11, SNMP ifIndex: 9
  Type: IPIP, Link-level type: IP-over-IP, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: irb, Enabled, Physical link is Up
  Interface index: 134, SNMP ifIndex: 503
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:f0:f0, Hardware address: 00:05:86:71:f0:f0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: lo0, Enabled, Physical link is Up
  Interface index: 6, SNMP ifIndex: 6
  Type: Loopback, MTU: Unlimited
  Device flags   : Present Running Loopback
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 4052
    Output packets: 4052

  Logical interface lo0.16384 (Index 324) (SNMP ifIndex 21)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 672
    Output packets: 672
    Protocol inet, MTU: Unlimited
      Addresses
        Local: 127.0.0.1

  Logical interface lo0.16385 (Index 325) (SNMP ifIndex 22)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 3376
    Output packets: 3376
    Protocol inet, MTU: Unlimited
      Addresses, Flags: Is-Default Is-Primary
        Local: 128.0.0.1
      Addresses
        Local: 128.0.0.4
    Protocol inet6, MTU: Unlimited
        Local: fe80::212:f:fc00:1a

  Logical interface lo0.32768 (Index 320) (SNMP ifIndex 250)
    Flags: Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0

Physical interface: lsi, Enabled, Physical link is Up
  Interface index: 4, SNMP ifIndex: 4
  Type: Software-Pseudo, Link-level type: LSI, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: mtun, Enabled, Physical link is Up
  Interface index: 64, SNMP ifIndex: 12
  Type: Multicast-GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: pimd, Enabled, Physical link is Up
  Interface index: 26, SNMP ifIndex: 11
  Type: PIMD, Link-level type: PIM-Decapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pime, Enabled, Physical link is Up
  Interface index: 25, SNMP ifIndex: 10
  Type: PIME, Link-level type: PIM-Encapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pip0, Enabled, Physical link is Up
  Interface index: 132, SNMP ifIndex: 504
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:f0:b0, Hardware address: 00:05:86:71:f0:b0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: pp0, Enabled, Physical link is Up
  Interface index: 133, SNMP ifIndex: 505
  Type: PPPoE, Link-level type: PPPoE, MTU: 1532
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None

Physical interface: tap, Enabled, Physical link is Up
  Interface index: 12, SNMP ifIndex: 7
  Type: Software-Pseudo, Link-level type: Interface-Specific, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: vtep, Enabled, Physical link is Up
  Interface index: 135, SNMP ifIndex: 506
  Type: Software-Pseudo, Link-level type: VxLAN-Tunnel-Endpoint, MTU: 1600, Speed: Unlimited
  Device flags   : Present Running
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

