Interface Ethernet1 detected 0 LLDP neighbors:

Interface Ethernet2 detected 0 LLDP neighbors:

Interface Ethernet3 detected 1 LLDP neighbors:

  Neighbor 0005.8671.f0c0/ge-0/0/10, age 8 seconds
  Discovered 18:52:08 ago; Last changed 18:52:08 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.f0c0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/10"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/10"
    - System Name: "sjc-ce01"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet4 detected 1 LLDP neighbors:

  Neighbor 0005.8671.9ec0/ge-0/0/10, age 1 seconds
  Discovered 18:52:02 ago; Last changed 18:52:02 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.9ec0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/10"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/10"
    - System Name: "sjc-ce02"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet5 detected 1 LLDP neighbors:

  Neighbor 0003.00e2.8008/Ethernet4, age 22 seconds
  Discovered 18:51:44 ago; Last changed 18:51:44 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0003.00e2.8008
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc301"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.61
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet6 detected 1 LLDP neighbors:

  Neighbor 0004.00af.d84d/Ethernet4, age 16 seconds
  Discovered 18:52:09 ago; Last changed 18:52:09 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0004.00af.d84d
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc302"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.62
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet7 detected 1 LLDP neighbors:

  Neighbor 0005.0030.bee3/Ethernet4, age 5 seconds
  Discovered 18:51:57 ago; Last changed 18:51:57 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.0030.bee3
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc303"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.63
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet8 detected 1 LLDP neighbors:

  Neighbor 0006.000b.1975/Ethernet4, age 13 seconds
  Discovered 18:52:06 ago; Last changed 18:52:06 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0006.000b.1975
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc304"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.64
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet9 detected 1 LLDP neighbors:

  Neighbor 0007.00cc.a553/Ethernet4, age 5 seconds
  Discovered 18:52:00 ago; Last changed 18:52:00 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0007.00cc.a553
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc305"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.65
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet10 detected 1 LLDP neighbors:

  Neighbor 0008.00cd.0130/Ethernet4, age 7 seconds
  Discovered 18:51:57 ago; Last changed 18:51:57 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0008.00cd.0130
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc306"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.66
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet11 detected 1 LLDP neighbors:

  Neighbor 0009.00ad.a12e/Ethernet4, age 11 seconds
  Discovered 18:52:05 ago; Last changed 18:52:05 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0009.00ad.a12e
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc307"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.67
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet12 detected 1 LLDP neighbors:

  Neighbor 0010.00f8.b12d/Ethernet4, age 13 seconds
  Discovered 18:52:07 ago; Last changed 18:52:07 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0010.00f8.b12d
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc308"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.68
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet13 detected 1 LLDP neighbors:

  Neighbor 0011.0017.612b/Ethernet4, age 3 seconds
  Discovered 18:51:51 ago; Last changed 18:51:51 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0011.0017.612b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc309"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.69
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet14 detected 1 LLDP neighbors:

  Neighbor 0012.00e4.0cbe/Ethernet4, age 4 seconds
  Discovered 18:52:02 ago; Last changed 18:52:02 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0012.00e4.0cbe
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc310"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.70
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet15 detected 1 LLDP neighbors:

  Neighbor 0013.004a.310b/Ethernet4, age 19 seconds
  Discovered 18:51:45 ago; Last changed 18:51:45 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0013.004a.310b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc311"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.71
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet16 detected 1 LLDP neighbors:

  Neighbor 0014.00f4.327c/Ethernet4, age 28 seconds
  Discovered 18:51:56 ago; Last changed 18:51:56 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0014.00f4.327c
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc312"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.72
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet17 detected 0 LLDP neighbors:

Interface Ethernet18 detected 1 LLDP neighbors:

  Neighbor 0001.006b.ea12/Ethernet18, age 9 seconds
  Discovered 18:52:05 ago; Last changed 18:52:05 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0001.006b.ea12
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet18"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-dist07"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.107
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet19 detected 0 LLDP neighbors:

Interface Management1 detected 0 LLDP neighbors:

