! Command: show running-config
! device: sjc-dc12-dist05 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-dist05
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1161-1170 priority 4096
!
!
no aaa root
!
!
vlan 1161-1170
!
vrf definition DEVZONE1
   rd 2:103
!
interface Ethernet1
   no switchport
   ip address 10.100.0.20/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   no switchport
   vrf forwarding DEVZONE1
   ip address 10.115.5.14/31
!
interface Ethernet4
   no switchport
   vrf forwarding DEVZONE1
   ip address 10.115.5.26/31
!
interface Ethernet5
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet6
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet7
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet8
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet9
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet10
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet11
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet12
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet13
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet14
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet15
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet16
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   switchport trunk allowed vlan 1161-1170
   switchport mode trunk
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.117.255.105/32
!
interface Management1
   ip address 10.117.38.75/24
!
interface Vlan1161
   vrf forwarding DEVZONE1
   ip address 10.117.161.2/24
   ip virtual-router address 10.117.161.1
!
interface Vlan1162
   vrf forwarding DEVZONE1
   ip address 10.117.162.2/24
   ip virtual-router address 10.117.162.1
!
interface Vlan1163
   vrf forwarding DEVZONE1
   ip address 10.117.163.2/24
   ip virtual-router address 10.117.163.1
!
interface Vlan1164
   vrf forwarding DEVZONE1
   ip address 10.117.164.2/24
   ip virtual-router address 10.117.164.1
!
interface Vlan1165
   vrf forwarding DEVZONE1
   ip address 10.117.165.2/24
   ip virtual-router address 10.117.165.1
!
interface Vlan1166
   vrf forwarding DEVZONE1
   ip address 10.117.166.2/24
   ip virtual-router address 10.117.166.1
!
interface Vlan1167
   vrf forwarding DEVZONE1
   ip address 10.117.167.2/24
   ip virtual-router address 10.117.167.1
!
interface Vlan1168
   vrf forwarding DEVZONE1
   ip address 10.117.168.2/24
   ip virtual-router address 10.117.168.1
!
interface Vlan1169
   vrf forwarding DEVZONE1
   ip address 10.117.169.2/24
   ip virtual-router address 10.117.169.1
!
interface Vlan1170
   vrf forwarding DEVZONE1
   ip address 10.117.170.2/24
   ip virtual-router address 10.117.170.1
!
ip virtual-router mac-address 00:1c:73:00:00:03
!
ip routing
ip routing vrf DEVZONE1
!
route-map TAG-OSPF permit 10
   set tag 100103
!
router ospf 1 vrf DEVZONE1
   router-id 10.117.255.105
   redistribute connected route-map TAG-OSPF
   network 10.115.5.14/31 area 0.0.0.0
   network 10.115.5.26/31 area 0.0.0.0
   network 10.117.162.0/24 area 0.0.0.0
   max-lsa 12000
!
!
end
