Interface GigabitEthernet0/0 "GigabitEthernet0/0", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	MAC address 0004.0000.0052, MTU 1500
	IP address 10.100.0.9, subnet mask 255.255.255.248
	348805 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	0 L2 decode drops
	6923165 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 3 interface resets
	0 late collisions, 0 deferred
	1 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (502/438)
	output queue (blocks free curr/low): hardware (511/502)
  Traffic Statistics for "GigabitEthernet0/0":
	341151 packets input, 15391707 bytes
	6914908 packets output, 743575235 bytes
	28 packets dropped
      1 minute input rate 0 pkts/sec,  11 bytes/sec
      1 minute output rate 6 pkts/sec,  633 bytes/sec
      1 minute drop rate, 0 pkts/sec
      5 minute input rate 0 pkts/sec,  9 bytes/sec
      5 minute output rate 5 pkts/sec,  630 bytes/sec
      5 minute drop rate, 0 pkts/sec
  Control Point Interface States:
	Interface number is 3
	Interface config status is active
	Interface state is active
Interface GigabitEthernet0/1 "", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	Available but not configured via nameif
	MAC address 0004.0000.0053, MTU not set
	IP address unassigned
	2 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	0 L2 decode drops
	3655 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 3 interface resets
	0 late collisions, 0 deferred
	2 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (511/511)
	output queue (blocks free curr/low): hardware (511/509)
  Control Point Interface States:
	Interface number is 4
	Interface config status is active
	Interface state is active
Interface GigabitEthernet0/1.107 "outside", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	VLAN identifier 107
	MAC address 0004.0000.0053, MTU 1500
	IP address 10.110.3.77, subnet mask 255.255.255.248
  Traffic Statistics for "outside":
	0 packets input, 0 bytes
	1242 packets output, 173768 bytes
	0 packets dropped
  Control Point Interface States:
	Interface number is 9
	Interface config status is active
	Interface state is active
  Control Point Vlan107 States:
	Interface vlan config status is active
	Interface vlan state is UP
Interface GigabitEthernet0/1.108 "inside", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	VLAN identifier 108
	MAC address 0004.0000.0053, MTU 1500
	IP address 10.110.3.85, subnet mask 255.255.255.248
  Traffic Statistics for "inside":
	0 packets input, 0 bytes
	1242 packets output, 173768 bytes
	0 packets dropped
  Control Point Interface States:
	Interface number is 10
	Interface config status is active
	Interface state is active
  Control Point Vlan108 States:
	Interface vlan config status is active
	Interface vlan state is UP
Interface GigabitEthernet0/2 "", is administratively down, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	Available but not configured via nameif
	MAC address 0004.0000.0054, MTU not set
	IP address unassigned
	1043 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	21 L2 decode drops
	0 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 3 interface resets
	0 late collisions, 0 deferred
	511 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (511/511)
	output queue (blocks free curr/low): hardware (511/511)
  Control Point Interface States:
	Interface number is 5
	Interface config status is not active
	Interface state is not active
Interface GigabitEthernet0/3 "LANFAIL", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	Description: LAN/STATE Failover Interface
	MAC address 0004.0000.0055, MTU 1500
	IP address 10.100.10.70, subnet mask 255.255.255.252
	3810621 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	0 L2 decode drops
	3290537 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 2 interface resets
	0 late collisions, 0 deferred
	2 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (507/456)
	output queue (blocks free curr/low): hardware (511/505)
  Traffic Statistics for "LANFAIL":
	3810569 packets input, 589939160 bytes
	3289237 packets output, 421378604 bytes
	0 packets dropped
      1 minute input rate 3 pkts/sec,  500 bytes/sec
      1 minute output rate 2 pkts/sec,  367 bytes/sec
      1 minute drop rate, 0 pkts/sec
      5 minute input rate 3 pkts/sec,  509 bytes/sec
      5 minute output rate 2 pkts/sec,  369 bytes/sec
      5 minute drop rate, 0 pkts/sec
  Control Point Interface States:
	Interface number is 6
	Interface config status is active
	Interface state is active
Interface GigabitEthernet0/4 "", is administratively down, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	Available but not configured via nameif
	MAC address 0004.0000.0056, MTU not set
	IP address unassigned
	2 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	0 L2 decode drops
	0 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 2 interface resets
	0 late collisions, 0 deferred
	2 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (511/511)
	output queue (blocks free curr/low): hardware (511/511)
  Control Point Interface States:
	Interface number is 7
	Interface config status is not active
	Interface state is not active
Interface Management0/0 "management", is up, line protocol is up
  Hardware is i82540EM rev03, BW 1000 Mbps, DLY 10 usec
	Auto-Duplex(Full-duplex), Auto-Speed(1000 Mbps)
	Input flow control is unsupported, output flow control is off
	MAC address 0004.0000.0051, MTU 1500
	IP address 10.110.37.202, subnet mask 255.255.255.0
	2 packets input, 0 bytes, 0 no buffer
	Received 0 broadcasts, 0 runts, 0 giants
	0 input errors, 0 CRC, 0 frame, 0 overrun, 0 ignored, 0 abort
	0 pause input, 0 resume input
	0 L2 decode drops
	203849 packets output, 0 bytes, 0 underruns
	0 pause output, 0 resume output
	0 output errors, 0 collisions, 2 interface resets
	0 late collisions, 0 deferred
	0 input reset drops, 0 output reset drops
	input queue (blocks free curr/low): hardware (511/511)
	output queue (blocks free curr/low): hardware (511/506)
  Traffic Statistics for "management":
	0 packets input, 0 bytes
	203849 packets output, 22052220 bytes
	0 packets dropped
      1 minute input rate 0 pkts/sec,  0 bytes/sec
      1 minute output rate 0 pkts/sec,  21 bytes/sec
      1 minute drop rate, 0 pkts/sec
      5 minute input rate 0 pkts/sec,  0 bytes/sec
      5 minute output rate 0 pkts/sec,  21 bytes/sec
      5 minute drop rate, 0 pkts/sec
	Management-only interface. Blocked 0 through-the-device packets
		0 IPv4 packets originated from management network
		0 IPv4 packets destined to management network
		0 IPv6 packets originated from management network
		0 IPv6 packets destined to management network
  Control Point Interface States:
	Interface number is 2
	Interface config status is active
	Interface state is active

