show lldp neighbors | no-more
Local Interface    Parent Interface    Chassis Id          Port info          System Name
ge-0/0/6           -                   00:05:86:71:67:c0   ge-0/0/3           sjc-internet        
ge-0/0/4           ae0                 00:05:86:71:9e:c0   ge-0/0/6           sjc-ce02            
ge-0/0/3           ae1                 00:05:86:71:f0:c0   ge-0/0/19          sjc-ce01            
ge-0/0/2           ae1                 00:05:86:71:f0:c0   ge-0/0/6           sjc-ce01            


LLDP nbr -- interface ge-0/0/6
LLDP Neighbor Information:
Local Information:
Index: 5 Time to live: 40 Time mark: Thu Aug 31 22:56:52 2017 Age: 2 secs 
Local Interface    : ge-0/0/6
Parent Interface   : -
Local Port ID      : 519
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:67:c0
Port type          : Interface name
Port ID            : ge-0/0/3
Port description   : To SJC-ISP-EDGE02
System name        : sjc-internet
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x1), Aggregation Port ID (0)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/4
LLDP Neighbor Information:
Local Information:
Index: 1 Time to live: 40 Time mark: Thu Aug 31 22:56:51 2017 Age: 3 secs 
Local Interface    : ge-0/0/4
Parent Interface   : ae0
Local Port ID      : 517
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:9e:c0
Port type          : Interface name
Port ID            : ge-0/0/6
Port description   : ge-0/0/6
System name        : sjc-ce02
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (523)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/3
LLDP Neighbor Information:
Local Information:
Index: 4 Time to live: 40 Time mark: Thu Aug 31 22:56:51 2017 Age: 3 secs 
Local Interface    : ge-0/0/3
Parent Interface   : ae1
Local Port ID      : 516
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:f0:c0
Port type          : Interface name
Port ID            : ge-0/0/19
Port description   : ge-0/0/19
System name        : sjc-ce01
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (524)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3




LLDP nbr -- interface ge-0/0/2
LLDP Neighbor Information:
Local Information:
Index: 3 Time to live: 40 Time mark: Thu Aug 31 22:56:48 2017 Age: 6 secs 
Local Interface    : ge-0/0/2
Parent Interface   : ae1
Local Port ID      : 515
Ageout Count      : 0

Neighbour Information:
Chassis type       : Mac address
Chassis ID         : 00:05:86:71:f0:c0
Port type          : Interface name
Port ID            : ge-0/0/6
Port description   : ge-0/0/6
System name        : sjc-ce01
  
System Description : Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC 


System capabilities 
        Supported: Bridge Router 
        Enabled  : Bridge Router 

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : MAC/PHY Configuration/Status (1)
       Info     : Autonegotiation [supported, enabled (0x3)], PMD Autonegotiation Capability (0x1d6c), MAU Type (0x0)
       Index    : 1

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Link Aggregation (3)
       Info     : Aggregation Status (0x3), Aggregation Port ID (524)
       Index    : 2

Organization Info
       OUI      : IEEE 802.3 Private (0x00120f)
       Subtype  : Maximum Frame Size (4)
       Info     : MTU Size (1514)
       Index    : 3



