Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  Internet address is 10.100.0.16/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     74534 packets input, 6040066 bytes
     Received 13 broadcasts, 68 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     232961 packets output, 50523612 bytes
     Sent 2 broadcasts, 120210 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     168377 packets input, 190864644 bytes
     Received 12 broadcasts, 168273 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     194218 packets output, 123597285 bytes
     Sent 2 broadcasts, 194126 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.8/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 49 seconds
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     169121 packets input, 191140273 bytes
     Received 13 broadcasts, 169017 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     194861 packets output, 123636360 bytes
     Sent 1 broadcasts, 194769 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.16/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 48 seconds
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     175155 packets input, 191695540 bytes
     Received 12 broadcasts, 174976 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     255372 packets output, 207496673 bytes
     Sent 2 broadcasts, 255204 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.24/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 48 seconds
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     175385 packets input, 191794253 bytes
     Received 12 broadcasts, 175206 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     255583 packets output, 207509700 bytes
     Sent 3 broadcasts, 255415 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.32/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     171702 packets input, 191398950 bytes
     Received 11 broadcasts, 171523 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     251799 packets output, 206671853 bytes
     Sent 3 broadcasts, 251631 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.40/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     170831 packets input, 191254789 bytes
     Received 12 broadcasts, 170652 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     250907 packets output, 206631338 bytes
     Sent 2 broadcasts, 250739 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.48/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     175438 packets input, 191928658 bytes
     Received 12 broadcasts, 175259 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     255789 packets output, 208358187 bytes
     Sent 2 broadcasts, 255585 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.56/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 46 seconds
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     172585 packets input, 190916774 bytes
     Received 12 broadcasts, 171914 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     252439 packets output, 208049155 bytes
     Sent 2 broadcasts, 252247 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.64/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 46 seconds
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     174227 packets input, 191548113 bytes
     Received 12 broadcasts, 174047 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     254473 packets output, 208345578 bytes
     Sent 3 broadcasts, 254293 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.72/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 46 seconds
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     170859 packets input, 191219748 bytes
     Received 13 broadcasts, 170679 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     250952 packets output, 206763888 bytes
     Sent 2 broadcasts, 250784 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.80/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 45 seconds
Ethernet12 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     171303 packets input, 191169664 bytes
     Received 13 broadcasts, 171123 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     251501 packets output, 206779497 bytes
     Sent 2 broadcasts, 251333 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet12.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.88/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 45 seconds
Ethernet13 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     173264 packets input, 191775050 bytes
     Received 13 broadcasts, 173083 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     253362 packets output, 207892764 bytes
     Sent 3 broadcasts, 253181 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet13.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.96/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 45 seconds
Ethernet14 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     172507 packets input, 191495625 bytes
     Received 12 broadcasts, 172327 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     252667 packets output, 208023707 bytes
     Sent 3 broadcasts, 252493 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet14.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.104/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet15 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     741476 packets input, 863531866 bytes
     Received 25 broadcasts, 740684 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     797267 packets output, 948572524 bytes
     Sent 10 broadcasts, 796505 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet15.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.1/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet15.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.5/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet15.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.9/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet15.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.13/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet15.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.17/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet16 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0000.00a7 (bia 0001.0000.00a7)
  Member of Port-Channel10
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:02:05 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     83471 packets input, 17515842 bytes
     Received 12 broadcasts, 83445 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1684259 packets output, 598371270 bytes
     Sent 3 broadcasts, 1615968 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet17 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0000.00a8 (bia 0001.0000.00a8)
  Member of Port-Channel11
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     224678 packets input, 31413480 bytes
     Received 474 broadcasts, 210261 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     2062008 packets output, 1106148307 bytes
     Sent 13 broadcasts, 1973568 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     174985 packets input, 191783548 bytes
     Received 12 broadcasts, 174805 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     254890 packets output, 207293063 bytes
     Sent 3 broadcasts, 254722 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.1.0/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet19 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0000.00aa (bia 0001.0000.00aa)
  Member of Port-Channel11
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     1360305 packets input, 155106742 bytes
     Received 4356 broadcasts, 1286785 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1321912 packets output, 175815147 bytes
     Sent 0 broadcasts, 1321912 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet20 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0000.00ab (bia 0001.0000.00ab)
  Member of Port-Channel10
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     1501767 packets input, 170067192 bytes
     Received 4826 broadcasts, 1413779 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1699178 packets output, 683486092 bytes
     Sent 10 broadcasts, 1679586 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet21 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 21 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     73 packets input, 5776 bytes
     Received 11 broadcasts, 62 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     120223 packets output, 21998554 bytes
     Sent 0 broadcasts, 120223 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0001.0000.007f (bia 0001.0000.007f)
  Internet address is 10.110.37.25/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 31 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     120209 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Port-Channel10 is up, line protocol is up (connected)
  Hardware is Port-Channel, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured 
  Active members in this channel: 2
  ... Ethernet16 , Full-duplex, Unconfigured
  ... Ethernet20 , Full-duplex, Unconfigured
  Fallback mode is: off
  Up 13 days, 21 hours, 49 minutes, 39 seconds
  2 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 1.22 kbps (- with framing overhead), 1 packets/sec
  5 minutes output rate 8.57 kbps (- with framing overhead), 3 packets/sec
     1585071 packets input, 187568856 bytes
     Received 4814 broadcasts, 1497081 multicast
     0 input errors, 0 input discards
     3383345 packets output, 1281844124 bytes
     Sent 13 broadcasts, 3295462 multicast
     0 output errors, 0 output discards
Port-Channel10.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.32/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 38 seconds
Port-Channel10.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.36/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel10.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.40/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel10.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.44/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel10.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.48/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel11 is up, line protocol is up (connected)
  Hardware is Port-Channel, address is 0001.0071.ab80
  IP MTU 1500 bytes
  Full-duplex, Unconfigured 
  Active members in this channel: 2
  ... Ethernet17 , Full-duplex, Unconfigured
  ... Ethernet19 , Full-duplex, Unconfigured
  Fallback mode is: off
  Up 13 days, 21 hours, 49 minutes, 39 seconds
  2 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 1.21 kbps (- with framing overhead), 1 packets/sec
  5 minutes output rate 8.56 kbps (- with framing overhead), 3 packets/sec
     1584817 packets input, 186505924 bytes
     Received 4806 broadcasts, 1496904 multicast
     0 input errors, 0 input discards
     3383829 packets output, 1281948797 bytes
     Sent 13 broadcasts, 3295391 multicast
     0 output errors, 0 output discards
Port-Channel11.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.64/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 38 seconds
Port-Channel11.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.68/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel11.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.72/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel11.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.76/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
Port-Channel11.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0001.0071.ab80
  Internet address is 10.110.2.80/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 39 seconds
