! Command: show running-config
! device: sjc-dc12-acc102 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-acc102
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1131-1140 priority 61440
!
!
no aaa root
!
!
vlan 1131-1140
!
interface Ethernet1
   no switchport
   ip address 10.100.0.152/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet4
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet5
   switchport trunk native vlan 1131
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet6
   switchport trunk native vlan 1131
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet7
   switchport trunk native vlan 1131
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet8
   no switchport
!
interface Ethernet9
   no switchport
!
interface Ethernet10
   no switchport
!
interface Ethernet11
   no switchport
!
interface Loopback0
   ip address 10.117.255.22/32
!
interface Management1
   ip address 10.117.38.24/24
!
ip routing
!
!
end
