Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  Internet address is 10.100.0.72/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     28334 packets input, 2527986 bytes
     Received 2 broadcasts, 50 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     96856 packets output, 19597525 bytes
     Sent 3 broadcasts, 40122 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     12 packets input, 768 bytes
     Received 0 broadcasts, 12 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40130 packets output, 7259943 bytes
     Sent 0 broadcasts, 40130 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.000a (bia 0019.0000.000a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     10142521 packets input, 842824186 bytes
     Received 801953 broadcasts, 9340455 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     43060 packets output, 7581307 bytes
     Sent 54 broadcasts, 43006 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.000c (bia 0019.0000.000c)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     10173410 packets input, 845017884 bytes
     Received 801907 broadcasts, 9371303 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     43156 packets output, 7587169 bytes
     Sent 53 broadcasts, 43098 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.000e (bia 0019.0000.000e)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10186606 packets output, 842308811 bytes
     Sent 801971 broadcasts, 9384528 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.0010 (bia 0019.0000.0010)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     6 packets input, 384 bytes
     Received 0 broadcasts, 6 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10186608 packets output, 842308923 bytes
     Sent 801971 broadcasts, 9384530 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.0012 (bia 0019.0000.0012)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10186609 packets output, 842308979 bytes
     Sent 801971 broadcasts, 9384531 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:06:17 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40139 packets output, 7260447 bytes
     Sent 0 broadcasts, 40139 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     4 packets input, 256 bytes
     Received 0 broadcasts, 4 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40141 packets output, 7260684 bytes
     Sent 0 broadcasts, 40141 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40128 packets output, 7300057 bytes
     Sent 0 broadcasts, 40128 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0060.a237
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 5 minutes, 45 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     5 packets input, 320 bytes
     Received 0 broadcasts, 5 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40128 packets output, 7299931 bytes
     Sent 0 broadcasts, 40128 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.117.255.11/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 50 minutes, 51 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0019.0000.0004 (bia 0019.0000.0004)
  Internet address is 10.117.38.21/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 1 minutes, 34 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40104 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
