Physical interface: ge-0/0/0, Enabled, Physical link is Up
  Interface index: 139, SNMP ifIndex: 513
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:04, Hardware address: 00:08:00:00:00:04
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 1536 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/0.0 (Index 329) (SNMP ifIndex 525)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 36470
    Output packets: 146730
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.100.0.50/31, Local: 10.100.0.50
    Protocol iso, MTU: 1497
      Flags: Is-Primary
    Protocol multiservice, MTU: Unlimited
      Flags: Is-Primary

Physical interface: lc-0/0/0, Enabled, Physical link is Up
  Interface index: 136, SNMP ifIndex: 507
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-0/0/0.32769 (Index 326) (SNMP ifIndex 508)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited
      Flags: Is-Primary

Physical interface: pfe-0/0/0, Enabled, Physical link is Up
  Interface index: 138, SNMP ifIndex: 511
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-0/0/0.16383 (Index 328) (SNMP ifIndex 512)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
      Flags: None

Physical interface: pfh-0/0/0, Enabled, Physical link is Up
  Interface index: 137, SNMP ifIndex: 509
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfh-0/0/0.16383 (Index 327) (SNMP ifIndex 510)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

Physical interface: ge-0/0/1, Enabled, Physical link is Up
  Interface index: 140, SNMP ifIndex: 514
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:05, Hardware address: 00:08:00:00:00:05
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 432 bps (0 pps)
  Output rate    : 936 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/1.0 (Index 330) (SNMP ifIndex 539)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 727878
    Output packets: 1196070
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.20/30, Local: 10.10.1.22, Broadcast: 10.10.1.23
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
      Flags: Is-Primary
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/2, Enabled, Physical link is Up
  Interface index: 141, SNMP ifIndex: 515
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:06, Hardware address: 00:08:00:00:00:06
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 424 bps (0 pps)
  Output rate    : 1096 bps (1 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/2.0 (Index 331) (SNMP ifIndex 540)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 746970
    Output packets: 1214649
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.28/30, Local: 10.10.1.30, Broadcast: 10.10.1.31
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/3, Enabled, Physical link is Up
  Interface index: 142, SNMP ifIndex: 516
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:07, Hardware address: 00:08:00:00:00:07
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 984 bps (1 pps)
  Output rate    : 600 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/3.0 (Index 332) (SNMP ifIndex 541)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 1300777
    Output packets: 774149
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.4/30, Local: 10.10.1.6, Broadcast: 10.10.1.7
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/4, Enabled, Physical link is Up
  Interface index: 143, SNMP ifIndex: 517
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:08, Hardware address: 00:08:00:00:00:08
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 856 bps (1 pps)
  Output rate    : 552 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/4.0 (Index 333) (SNMP ifIndex 542)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 1259842
    Output packets: 793738
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.10.1.12/30, Local: 10.10.1.14, Broadcast: 10.10.1.15
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/5, Administratively down, Physical link is Down
  Interface index: 144, SNMP ifIndex: 518
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:09, Hardware address: 00:08:00:00:00:09
  Last flapped   : 2017-08-22 06:38:57 UTC (1w2d 16:17 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/5.0 (Index 334) (SNMP ifIndex 543)
    Flags: Device-Down SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 295336
    Output packets: 220452
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Dest-route-down Is-Preferred Is-Primary
        Destination: 10.10.1.36/30, Local: 10.10.1.38, Broadcast: 10.10.1.39
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/6, Administratively down, Physical link is Down
  Interface index: 145, SNMP ifIndex: 519
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:0a, Hardware address: 00:08:00:00:00:0a
  Last flapped   : 2017-08-22 06:38:57 UTC (1w2d 16:17 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-0/0/6.0 (Index 335) (SNMP ifIndex 544)
    Flags: Device-Down SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 310198
    Output packets: 220722
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Dest-route-down Is-Preferred Is-Primary
        Destination: 10.10.1.44/30, Local: 10.10.1.46, Broadcast: 10.10.1.47
    Protocol iso, MTU: 1497
    Protocol mpls, MTU: 1488, Maximum labels: 3
    Protocol multiservice, MTU: Unlimited

Physical interface: ge-0/0/7, Enabled, Physical link is Up
  Interface index: 146, SNMP ifIndex: 520
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:0b, Hardware address: 00:08:00:00:00:0b
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/8, Enabled, Physical link is Up
  Interface index: 147, SNMP ifIndex: 521
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:08:00:00:00:0c, Hardware address: 00:08:00:00:00:0c
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/9, Enabled, Physical link is Down
  Interface index: 148, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:09, Hardware address: 00:05:86:71:a7:09
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/10, Enabled, Physical link is Down
  Interface index: 149, SNMP ifIndex: 526
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0a, Hardware address: 00:05:86:71:a7:0a
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/11, Enabled, Physical link is Down
  Interface index: 150, SNMP ifIndex: 527
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0b, Hardware address: 00:05:86:71:a7:0b
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/12, Enabled, Physical link is Down
  Interface index: 151, SNMP ifIndex: 528
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0c, Hardware address: 00:05:86:71:a7:0c
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/13, Enabled, Physical link is Down
  Interface index: 152, SNMP ifIndex: 529
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0d, Hardware address: 00:05:86:71:a7:0d
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/14, Enabled, Physical link is Down
  Interface index: 153, SNMP ifIndex: 530
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0e, Hardware address: 00:05:86:71:a7:0e
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/15, Enabled, Physical link is Down
  Interface index: 154, SNMP ifIndex: 531
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:0f, Hardware address: 00:05:86:71:a7:0f
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/16, Enabled, Physical link is Down
  Interface index: 155, SNMP ifIndex: 532
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:10, Hardware address: 00:05:86:71:a7:10
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/17, Enabled, Physical link is Down
  Interface index: 156, SNMP ifIndex: 533
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:11, Hardware address: 00:05:86:71:a7:11
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/18, Enabled, Physical link is Down
  Interface index: 157, SNMP ifIndex: 534
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:12, Hardware address: 00:05:86:71:a7:12
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/19, Enabled, Physical link is Down
  Interface index: 158, SNMP ifIndex: 535
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:13, Hardware address: 00:05:86:71:a7:13
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/20, Enabled, Physical link is Down
  Interface index: 159, SNMP ifIndex: 536
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:14, Hardware address: 00:05:86:71:a7:14
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/21, Enabled, Physical link is Down
  Interface index: 160, SNMP ifIndex: 537
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:15, Hardware address: 00:05:86:71:a7:15
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-0/0/22, Enabled, Physical link is Down
  Interface index: 161, SNMP ifIndex: 538
  Link-level type: Ethernet, MTU: 1514, MRU: 1522, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled
  Pad to minimum frame size: Disabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: 00:05:86:71:a7:16, Hardware address: 00:05:86:71:a7:16
  Last flapped   : 2017-08-18 00:52:49 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ae0, Enabled, Physical link is Down
  Interface index: 128, SNMP ifIndex: 523
  Link-level type: Ethernet, MTU: 1514, Speed: Unspecified, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:aa:c0, Hardware address: 00:05:86:71:aa:c0
  Last flapped   : 2017-08-18 00:52:01 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)

Physical interface: ae1, Enabled, Physical link is Down
  Interface index: 129, SNMP ifIndex: 524
  Link-level type: Ethernet, MTU: 1514, Speed: Unspecified, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled
  Pad to minimum frame size: Disabled
  Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Current address: 00:05:86:71:aa:c1, Hardware address: 00:05:86:71:aa:c1
  Last flapped   : 2017-08-18 00:52:01 UTC (1w6d 22:04 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)

Physical interface: cbp0, Enabled, Physical link is Up
  Interface index: 131, SNMP ifIndex: 501
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:a7:11, Hardware address: 00:05:86:71:a7:11
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: demux0, Enabled, Physical link is Up
  Interface index: 130, SNMP ifIndex: 502
  Type: Software-Pseudo, MTU: 9192, Clocking: 1
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: dsc, Enabled, Physical link is Up
  Interface index: 5, SNMP ifIndex: 5
  Type: Software-Pseudo, MTU: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: em1, Enabled, Physical link is Up
  Interface index: 9, SNMP ifIndex: 23
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 52:54:00:c8:ea:f9, Hardware address: 52:54:00:c8:ea:f9
  Last flapped   : Never
    Input packets : 511129223
    Output packets: 569812737

  Logical interface em1.0 (Index 3) (SNMP ifIndex 24)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 511129223
    Output packets: 569812737
    Protocol inet, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 172.16/16, Local: 172.16.0.1, Broadcast: 172.16.255.255
    Protocol inet6, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred
        Destination: fe80::/64, Local: fe80::5254:ff:fec8:eaf9

Physical interface: fxp0, Enabled, Physical link is Up
  Interface index: 8, SNMP ifIndex: 1
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Current address: 00:08:00:00:00:0d, Hardware address: 00:08:00:00:00:0d
  Last flapped   : 2017-08-18 00:52:04 UTC (1w6d 22:04 ago)
    Input packets : 20953
    Output packets: 0

Physical interface: gre, Enabled, Physical link is Up
  Interface index: 10, SNMP ifIndex: 8
  Type: GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: ipip, Enabled, Physical link is Up
  Interface index: 11, SNMP ifIndex: 9
  Type: IPIP, Link-level type: IP-over-IP, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: irb, Enabled, Physical link is Up
  Interface index: 134, SNMP ifIndex: 503
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:aa:f0, Hardware address: 00:05:86:71:aa:f0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: lo0, Enabled, Physical link is Up
  Interface index: 6, SNMP ifIndex: 6
  Type: Loopback, MTU: Unlimited
  Device flags   : Present Running Loopback
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 4050
    Output packets: 4050

  Logical interface lo0.0 (Index 336) (SNMP ifIndex 16)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Default Is-Primary
        Local: 10.10.0.2
    Protocol iso, MTU: Unlimited
      Addresses, Flags: Is-Default Is-Primary
        Local: 49.0001.0100.1000.0002

  Logical interface lo0.16384 (Index 324) (SNMP ifIndex 21)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 672
    Output packets: 672
    Protocol inet, MTU: Unlimited
      Addresses
        Local: 127.0.0.1

  Logical interface lo0.16385 (Index 325) (SNMP ifIndex 22)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 3378
    Output packets: 3378
    Protocol inet, MTU: Unlimited
      Addresses, Flags: Is-Default Is-Primary
        Local: 128.0.0.1
      Addresses
        Local: 128.0.0.4
    Protocol inet6, MTU: Unlimited
        Local: fe80::208:f:fc00:d

  Logical interface lo0.32768 (Index 320) (SNMP ifIndex 250)
    Flags: Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0

Physical interface: lsi, Enabled, Physical link is Up
  Interface index: 4, SNMP ifIndex: 4
  Type: Software-Pseudo, Link-level type: LSI, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: mtun, Enabled, Physical link is Up
  Interface index: 64, SNMP ifIndex: 12
  Type: Multicast-GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: pimd, Enabled, Physical link is Up
  Interface index: 26, SNMP ifIndex: 11
  Type: PIMD, Link-level type: PIM-Decapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pime, Enabled, Physical link is Up
  Interface index: 25, SNMP ifIndex: 10
  Type: PIME, Link-level type: PIM-Encapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pip0, Enabled, Physical link is Up
  Interface index: 132, SNMP ifIndex: 504
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: 00:05:86:71:aa:b0, Hardware address: 00:05:86:71:aa:b0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: pp0, Enabled, Physical link is Up
  Interface index: 133, SNMP ifIndex: 505
  Type: PPPoE, Link-level type: PPPoE, MTU: 1532
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None

Physical interface: tap, Enabled, Physical link is Up
  Interface index: 12, SNMP ifIndex: 7
  Type: Software-Pseudo, Link-level type: Interface-Specific, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: vtep, Enabled, Physical link is Up
  Interface index: 135, SNMP ifIndex: 506
  Type: Software-Pseudo, Link-level type: VxLAN-Tunnel-Endpoint, MTU: 1600, Speed: Unlimited
  Device flags   : Present Running
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

