Physical interface: ge-1/0/0, Enabled, Physical link is Up
  Interface index: 139, SNMP ifIndex: 552
  Link-level type: Ethernet, MTU: 1600, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:95, Hardware address: dc:38:e1:f8:fe:95
  Last flapped   : 2019-01-10 19:50:36 PST (08:13:30 ago)
  Input rate     : 968 bps (1 pps)
  Output rate    : 4080 bps (4 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-1/0/0.0 (Index 331) (SNMP ifIndex 622)
    Flags: Up SNMP-Traps 0x20024000 Encapsulation: Ethernet-Bridge
    Input packets : 71
    Output packets: 136
    Protocol eth-switch, MTU: 1600
      Flags: Is-Primary, Trunk-Mode

  Logical interface ge-1/0/0.32767 (Index 332) (SNMP ifIndex 624)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 1
    Output packets: 3
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: lc-1/0/0, Enabled, Physical link is Up
  Interface index: 136, SNMP ifIndex: 507
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-1/0/0.32769 (Index 327) (SNMP ifIndex 508)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited
      Flags: Is-Primary

Physical interface: pfe-1/0/0, Enabled, Physical link is Up
  Interface index: 138, SNMP ifIndex: 511
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-1/0/0.16383 (Index 328) (SNMP ifIndex 512)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
    Max nh cache: 0, New hold nh limit: 0, Curr nh cnt: 0, Curr new hold cnt: 0, NH drop cnt: 0
      Flags: None

Physical interface: pfh-1/0/0, Enabled, Physical link is Up
  Interface index: 137, SNMP ifIndex: 509
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfh-1/0/0.16383 (Index 329) (SNMP ifIndex 510)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

  Logical interface pfh-1/0/0.16384 (Index 330) (SNMP ifIndex 621)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: Is-Primary

Physical interface: ge-1/0/1, Enabled, Physical link is Up
  Interface index: 140, SNMP ifIndex: 553
  Link-level type: Ethernet, MTU: 1600, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:96, Hardware address: dc:38:e1:f8:fe:96
  Last flapped   : 2019-01-10 19:50:36 PST (08:13:30 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 3632 bps (4 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-1/0/1.0 (Index 333) (SNMP ifIndex 623)
    Flags: Up SNMP-Traps 0x20024000 Encapsulation: Ethernet-Bridge
    Input packets : 20
    Output packets: 186
    Protocol eth-switch, MTU: 1600
      Flags: Trunk-Mode

  Logical interface ge-1/0/1.32767 (Index 334) (SNMP ifIndex 625)
    Flags: Up SNMP-Traps 0x4004000 VLAN-Tag [ 0x0000.0 ]  Encapsulation: ENET2
    Input packets : 1
    Output packets: 2
    Protocol multiservice, MTU: Unlimited
      Flags: None

Physical interface: ge-1/0/2, Enabled, Physical link is Up
  Interface index: 141, SNMP ifIndex: 554
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:97, Hardware address: dc:38:e1:f8:fe:97
  Last flapped   : 2019-01-10 20:38:37 PST (07:25:29 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 1152 bps (1 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

  Logical interface ge-1/0/2.0 (Index 335) (SNMP ifIndex 627)
    Description: test_port
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Input packets : 0
    Output packets: 46
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 192.168.10/24, Local: 192.168.10.1, Broadcast: 192.168.10.255
    Protocol multiservice, MTU: Unlimited
      Flags: Is-Primary

Physical interface: ge-1/0/3, Enabled, Physical link is Up
  Interface index: 142, SNMP ifIndex: 555
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:98, Hardware address: dc:38:e1:f8:fe:98
  Last flapped   : 2019-01-10 19:50:36 PST (08:13:30 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/4, Enabled, Physical link is Up
  Interface index: 143, SNMP ifIndex: 556
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:99, Hardware address: dc:38:e1:f8:fe:99
  Last flapped   : 2019-01-10 21:45:54 PST (06:18:12 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/5, Enabled, Physical link is Down
  Interface index: 144, SNMP ifIndex: 557
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:9a, Hardware address: dc:38:e1:f8:fe:9a
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/6, Enabled, Physical link is Down
  Interface index: 145, SNMP ifIndex: 558
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:9b, Hardware address: dc:38:e1:f8:fe:9b
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/7, Enabled, Physical link is Up
  Interface index: 146, SNMP ifIndex: 549
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:9c, Hardware address: dc:38:e1:f8:fe:9c
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/8, Enabled, Physical link is Down
  Interface index: 147, SNMP ifIndex: 550
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:9d, Hardware address: dc:38:e1:f8:fe:9d
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/0/9, Enabled, Physical link is Up
  Interface index: 148, SNMP ifIndex: 551
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:fe:9e, Hardware address: dc:38:e1:f8:fe:9e
  Last flapped   : 2019-01-10 20:38:38 PST (07:25:28 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/0, Enabled, Physical link is Down
  Interface index: 149, SNMP ifIndex: 559
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3a, Hardware address: dc:38:e1:f8:ff:3a
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/1, Enabled, Physical link is Down
  Interface index: 150, SNMP ifIndex: 560
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3b, Hardware address: dc:38:e1:f8:ff:3b
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/2, Enabled, Physical link is Up
  Interface index: 151, SNMP ifIndex: 561
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3c, Hardware address: dc:38:e1:f8:ff:3c
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/3, Enabled, Physical link is Up
  Interface index: 152, SNMP ifIndex: 562
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3d, Hardware address: dc:38:e1:f8:ff:3d
  Last flapped   : 2019-01-11 03:19:42 PST (00:44:24 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/4, Enabled, Physical link is Up
  Interface index: 153, SNMP ifIndex: 563
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3e, Hardware address: dc:38:e1:f8:ff:3e
  Last flapped   : 2019-01-11 03:19:42 PST (00:44:24 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/5, Enabled, Physical link is Down
  Interface index: 154, SNMP ifIndex: 564
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:3f, Hardware address: dc:38:e1:f8:ff:3f
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/6, Enabled, Physical link is Down
  Interface index: 155, SNMP ifIndex: 565
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:40, Hardware address: dc:38:e1:f8:ff:40
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/7, Enabled, Physical link is Up
  Interface index: 156, SNMP ifIndex: 566
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:41, Hardware address: dc:38:e1:f8:ff:41
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : None
  Active defects : None
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/8, Enabled, Physical link is Down
  Interface index: 157, SNMP ifIndex: 567
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:42, Hardware address: dc:38:e1:f8:ff:42
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/1/9, Enabled, Physical link is Down
  Interface index: 158, SNMP ifIndex: 568
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:43, Hardware address: dc:38:e1:f8:ff:43
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/0, Enabled, Physical link is Down
  Interface index: 159, SNMP ifIndex: 576
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:df, Hardware address: dc:38:e1:f8:ff:df
  Last flapped   : 2019-01-10 17:30:25 PST (10:33:41 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/1, Enabled, Physical link is Down
  Interface index: 160, SNMP ifIndex: 577
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e0, Hardware address: dc:38:e1:f8:ff:e0
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/2, Enabled, Physical link is Down
  Interface index: 161, SNMP ifIndex: 578
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e1, Hardware address: dc:38:e1:f8:ff:e1
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/3, Enabled, Physical link is Down
  Interface index: 162, SNMP ifIndex: 569
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e2, Hardware address: dc:38:e1:f8:ff:e2
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/4, Enabled, Physical link is Down
  Interface index: 163, SNMP ifIndex: 570
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e3, Hardware address: dc:38:e1:f8:ff:e3
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/5, Enabled, Physical link is Down
  Interface index: 164, SNMP ifIndex: 571
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e4, Hardware address: dc:38:e1:f8:ff:e4
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/6, Enabled, Physical link is Down
  Interface index: 165, SNMP ifIndex: 572
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e5, Hardware address: dc:38:e1:f8:ff:e5
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/7, Enabled, Physical link is Down
  Interface index: 166, SNMP ifIndex: 573
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e6, Hardware address: dc:38:e1:f8:ff:e6
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/8, Enabled, Physical link is Down
  Interface index: 167, SNMP ifIndex: 574
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e7, Hardware address: dc:38:e1:f8:ff:e7
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/2/9, Enabled, Physical link is Down
  Interface index: 168, SNMP ifIndex: 575
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f8:ff:e8, Hardware address: dc:38:e1:f8:ff:e8
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/0, Enabled, Physical link is Down
  Interface index: 169, SNMP ifIndex: 579
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:84, Hardware address: dc:38:e1:f9:00:84
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/1, Enabled, Physical link is Down
  Interface index: 170, SNMP ifIndex: 580
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:85, Hardware address: dc:38:e1:f9:00:85
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/2, Enabled, Physical link is Down
  Interface index: 171, SNMP ifIndex: 581
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:86, Hardware address: dc:38:e1:f9:00:86
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/3, Enabled, Physical link is Down
  Interface index: 172, SNMP ifIndex: 582
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:87, Hardware address: dc:38:e1:f9:00:87
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/4, Enabled, Physical link is Down
  Interface index: 173, SNMP ifIndex: 583
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:88, Hardware address: dc:38:e1:f9:00:88
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/5, Enabled, Physical link is Down
  Interface index: 174, SNMP ifIndex: 584
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:89, Hardware address: dc:38:e1:f9:00:89
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/6, Enabled, Physical link is Down
  Interface index: 175, SNMP ifIndex: 585
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:8a, Hardware address: dc:38:e1:f9:00:8a
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/7, Enabled, Physical link is Down
  Interface index: 176, SNMP ifIndex: 586
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:8b, Hardware address: dc:38:e1:f9:00:8b
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/8, Enabled, Physical link is Down
  Interface index: 177, SNMP ifIndex: 587
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:8c, Hardware address: dc:38:e1:f9:00:8c
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: ge-1/3/9, Enabled, Physical link is Down
  Interface index: 178, SNMP ifIndex: 588
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 1000mbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Enabled, Auto-negotiation: Enabled, Remote fault: Online, Media type: Copper, Speed-negotiation: Disabled, Auto-MDIX: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:00:8d, Hardware address: dc:38:e1:f9:00:8d
  Last flapped   : 2019-01-10 06:17:34 PST (21:46:32 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  Interface transmit statistics: Disabled

Physical interface: lc-2/0/0, Enabled, Physical link is Up
  Interface index: 179, SNMP ifIndex: 513
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-2/0/0.32769 (Index 340) (SNMP ifIndex 514)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited

Physical interface: pfe-2/0/0, Enabled, Physical link is Up
  Interface index: 182, SNMP ifIndex: 516
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-2/0/0.16383 (Index 342) (SNMP ifIndex 517)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
    Max nh cache: 0, New hold nh limit: 0, Curr nh cnt: 0, Curr new hold cnt: 0, NH drop cnt: 0
      Flags: None

Physical interface: pfh-2/0/0, Enabled, Physical link is Up
  Interface index: 181, SNMP ifIndex: 515
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfh-2/0/0.16383 (Index 344) (SNMP ifIndex 534)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

  Logical interface pfh-2/0/0.16384 (Index 345) (SNMP ifIndex 626)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None

Physical interface: xe-2/0/0, Enabled, Physical link is Down
  Interface index: 184, SNMP ifIndex: 518
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2a, Hardware address: dc:38:e1:f9:01:2a
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/1, Enabled, Physical link is Down
  Interface index: 185, SNMP ifIndex: 519
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2b, Hardware address: dc:38:e1:f9:01:2b
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/2, Enabled, Physical link is Down
  Interface index: 186, SNMP ifIndex: 520
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2c, Hardware address: dc:38:e1:f9:01:2c
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/3, Enabled, Physical link is Down
  Interface index: 187, SNMP ifIndex: 521
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2d, Hardware address: dc:38:e1:f9:01:2d
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/4, Enabled, Physical link is Down
  Interface index: 188, SNMP ifIndex: 595
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2e, Hardware address: dc:38:e1:f9:01:2e
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/5, Enabled, Physical link is Down
  Interface index: 189, SNMP ifIndex: 593
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:2f, Hardware address: dc:38:e1:f9:01:2f
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/6, Enabled, Physical link is Down
  Interface index: 190, SNMP ifIndex: 594
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:30, Hardware address: dc:38:e1:f9:01:30
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/0/7, Enabled, Physical link is Down
  Interface index: 191, SNMP ifIndex: 596
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:31, Hardware address: dc:38:e1:f9:01:31
  Last flapped   : 2019-01-10 06:20:12 PST (21:43:54 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/0, Enabled, Physical link is Down
  Interface index: 192, SNMP ifIndex: 604
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:cf, Hardware address: dc:38:e1:f9:01:cf
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/1, Enabled, Physical link is Down
  Interface index: 193, SNMP ifIndex: 597
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d0, Hardware address: dc:38:e1:f9:01:d0
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/2, Enabled, Physical link is Down
  Interface index: 194, SNMP ifIndex: 598
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d1, Hardware address: dc:38:e1:f9:01:d1
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/3, Enabled, Physical link is Down
  Interface index: 195, SNMP ifIndex: 599
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d2, Hardware address: dc:38:e1:f9:01:d2
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/4, Enabled, Physical link is Down
  Interface index: 196, SNMP ifIndex: 600
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d3, Hardware address: dc:38:e1:f9:01:d3
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/5, Enabled, Physical link is Down
  Interface index: 197, SNMP ifIndex: 601
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d4, Hardware address: dc:38:e1:f9:01:d4
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/6, Enabled, Physical link is Down
  Interface index: 198, SNMP ifIndex: 602
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d5, Hardware address: dc:38:e1:f9:01:d5
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         1
  Interface transmit statistics: Disabled

Physical interface: xe-2/1/7, Enabled, Physical link is Down
  Interface index: 199, SNMP ifIndex: 603
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:01:d6, Hardware address: dc:38:e1:f9:01:d6
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: lc-2/2/0, Enabled, Physical link is Up
  Interface index: 180, SNMP ifIndex: 589
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface lc-2/2/0.32769 (Index 341) (SNMP ifIndex 590)
    Flags: Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol vpls, MTU: Unlimited

Physical interface: pfe-2/2/0, Enabled, Physical link is Up
  Interface index: 183, SNMP ifIndex: 591
  Speed: 800mbps
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface pfe-2/2/0.16383 (Index 343) (SNMP ifIndex 592)
    Flags: Up SNMP-Traps Encapsulation: ENET2
    Bandwidth: 0
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: None
    Protocol inet6, MTU: Unlimited
    Max nh cache: 0, New hold nh limit: 0, Curr nh cnt: 0, Curr new hold cnt: 0, NH drop cnt: 0
      Flags: None

Physical interface: xe-2/2/0, Enabled, Physical link is Down
  Interface index: 200, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:74, Hardware address: dc:38:e1:f9:02:74
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/1, Enabled, Physical link is Down
  Interface index: 201, SNMP ifIndex: 523
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:75, Hardware address: dc:38:e1:f9:02:75
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/2, Enabled, Physical link is Down
  Interface index: 202, SNMP ifIndex: 524
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:76, Hardware address: dc:38:e1:f9:02:76
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/3, Enabled, Physical link is Down
  Interface index: 203, SNMP ifIndex: 525
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:77, Hardware address: dc:38:e1:f9:02:77
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/4, Enabled, Physical link is Down
  Interface index: 204, SNMP ifIndex: 605
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:78, Hardware address: dc:38:e1:f9:02:78
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/5, Enabled, Physical link is Down
  Interface index: 205, SNMP ifIndex: 606
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:79, Hardware address: dc:38:e1:f9:02:79
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/6, Enabled, Physical link is Down
  Interface index: 206, SNMP ifIndex: 607
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:7a, Hardware address: dc:38:e1:f9:02:7a
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/2/7, Enabled, Physical link is Down
  Interface index: 207, SNMP ifIndex: 608
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:02:7b, Hardware address: dc:38:e1:f9:02:7b
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/0, Enabled, Physical link is Down
  Interface index: 208, SNMP ifIndex: 610
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:19, Hardware address: dc:38:e1:f9:03:19
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/1, Enabled, Physical link is Down
  Interface index: 209, SNMP ifIndex: 611
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1a, Hardware address: dc:38:e1:f9:03:1a
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/2, Enabled, Physical link is Down
  Interface index: 210, SNMP ifIndex: 612
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1b, Hardware address: dc:38:e1:f9:03:1b
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/3, Enabled, Physical link is Down
  Interface index: 211, SNMP ifIndex: 613
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1c, Hardware address: dc:38:e1:f9:03:1c
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/4, Enabled, Physical link is Down
  Interface index: 212, SNMP ifIndex: 614
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1d, Hardware address: dc:38:e1:f9:03:1d
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/5, Enabled, Physical link is Down
  Interface index: 213, SNMP ifIndex: 615
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1e, Hardware address: dc:38:e1:f9:03:1e
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/6, Enabled, Physical link is Down
  Interface index: 214, SNMP ifIndex: 616
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:1f, Hardware address: dc:38:e1:f9:03:1f
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: xe-2/3/7, Enabled, Physical link is Down
  Interface index: 215, SNMP ifIndex: 609
  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 10Gbps, BPDU Error: None, MAC-REWRITE Error: None, Loopback: None, Source filtering: Disabled, Flow control: Enabled
  Device flags   : Present Running Down
  Interface flags: Hardware-Down SNMP-Traps Internal: 0x4000
  Link flags     : None
  CoS queues     : 8 supported, 8 maximum usable queues
  Current address: dc:38:e1:f9:03:20, Hardware address: dc:38:e1:f9:03:20
  Last flapped   : 2019-01-10 06:20:17 PST (21:43:49 ago)
  Input rate     : 0 bps (0 pps)
  Output rate    : 0 bps (0 pps)
  Active alarms  : LINK
  Active defects : LINK
  PCS statistics                      Seconds
    Bit errors                             0
    Errored blocks                         0
  Interface transmit statistics: Disabled

Physical interface: cbp0, Enabled, Physical link is Up
  Interface index: 129, SNMP ifIndex: 502
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: dc:38:e1:f8:fc:11, Hardware address: dc:38:e1:f8:fc:11
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: demux0, Enabled, Physical link is Up
  Interface index: 128, SNMP ifIndex: 501
  Type: Software-Pseudo, MTU: 9192, Clocking: 1
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: dsc, Enabled, Physical link is Up
  Interface index: 5, SNMP ifIndex: 5
  Type: Software-Pseudo, MTU: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: em0, Enabled, Physical link is Up
  Interface index: 8, SNMP ifIndex: 17
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 02:00:00:00:00:04, Hardware address: 02:00:00:00:00:04
  Last flapped   : 2019-01-10 06:15:28 PST (21:48:38 ago)
    Input packets : 3980084
    Output packets: 3346167

  Logical interface em0.0 (Index 3) (SNMP ifIndex 18)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 3980032
    Output packets: 3346167
    Protocol inet, MTU: 1500
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred
        Destination: 10/8, Local: 10.0.0.4, Broadcast: 10.255.255.255
      Addresses, Flags: Preferred Kernel Is-Preferred
        Destination: 128/2, Local: 128.0.0.1, Broadcast: 191.255.255.255
      Addresses, Flags: Primary Is-Default Is-Primary
        Destination: 128/2, Local: 128.0.0.4, Broadcast: 191.255.255.255
    Protocol inet6, MTU: 1500
    Max nh cache: 100000, New hold nh limit: 100000, Curr nh cnt: 2, Curr new hold cnt: 0, NH drop cnt: 0
      Flags: Is-Primary
      Addresses, Flags: Is-Preferred
        Destination: fe80::/64, Local: fe80::200:ff:fe00:4
      Addresses, Flags: Is-Default Is-Preferred Is-Primary
        Destination: fec0::/64, Local: fec0::a:0:0:4
    Protocol tnp, MTU: 1500
      Flags: Primary, Is-Primary
      Addresses
        Local: 0x4

Physical interface: em1, Enabled, Physical link is Up
  Interface index: 9, SNMP ifIndex: 23
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 02:00:01:00:00:04, Hardware address: 02:00:01:00:00:04
  Last flapped   : 2019-01-10 06:15:28 PST (21:48:38 ago)
    Input packets : 0
    Output packets: 78529

  Logical interface em1.0 (Index 4) (SNMP ifIndex 24)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 0
    Output packets: 78529
    Protocol inet, MTU: 1500
      Flags: None
      Addresses, Flags: Is-Preferred
        Destination: 10/8, Local: 10.0.0.4, Broadcast: 10.255.255.255
      Addresses, Flags: Preferred Kernel Is-Preferred
        Destination: 128/2, Local: 128.0.0.1, Broadcast: 191.255.255.255
      Addresses, Flags: Primary Is-Primary
        Destination: 128/2, Local: 128.0.0.4, Broadcast: 191.255.255.255
    Protocol inet6, MTU: 1500
    Max nh cache: 100000, New hold nh limit: 100000, Curr nh cnt: 0, Curr new hold cnt: 0, NH drop cnt: 0
      Flags: None
      Addresses, Flags: Is-Preferred
        Destination: fe80::/64, Local: fe80::200:1ff:fe00:4
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: fec0::/64, Local: fec0::a:0:0:4
    Protocol tnp, MTU: 1500
      Flags: None
      Addresses
        Local: 0x4

Physical interface: esi, Enabled, Physical link is Up
  Interface index: 134, SNMP ifIndex: 617
  Type: Software-Pseudo, Link-level type: VxLAN-Tunnel-Endpoint, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: fxp0, Enabled, Physical link is Up
  Interface index: 64, SNMP ifIndex: 1
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514, Speed: 1000mbps
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Current address: 00:a0:a5:7f:66:7f, Hardware address: 00:a0:a5:7f:66:7f
  Last flapped   : 2019-01-10 06:15:28 PST (21:48:38 ago)
    Input packets : 452430
    Output packets: 747393

  Logical interface fxp0.0 (Index 5) (SNMP ifIndex 13)
    Flags: Up SNMP-Traps 0x4000000 Encapsulation: ENET2
    Input packets : 452409
    Output packets: 747393
    Protocol inet, MTU: 1500
      Flags: Sendbcast-pkt-to-re, Is-Primary
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.128.64/24, Local: 10.128.64.10, Broadcast: 10.128.64.255

Physical interface: gre, Enabled, Physical link is Up
  Interface index: 10, SNMP ifIndex: 8
  Type: GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: ipip, Enabled, Physical link is Up
  Interface index: 11, SNMP ifIndex: 9
  Type: IPIP, Link-level type: IP-over-IP, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: irb, Enabled, Physical link is Up
  Interface index: 132, SNMP ifIndex: 505
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: dc:38:e1:f9:03:f0, Hardware address: dc:38:e1:f9:03:f0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface irb.30 (Index 336) (SNMP ifIndex 628)
    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2
    Bandwidth: 1000mbps
    Routing Instance: default-switch Bridging Domain: vl30
    Input packets : 40
    Output packets: 50
    Protocol inet, MTU: 1582
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 192.168.59/24, Local: 192.168.59.2, Broadcast: 192.168.59.255
    Protocol multiservice, MTU: 1582

  Logical interface irb.214 (Index 337) (SNMP ifIndex 629)
    Flags: Up SNMP-Traps 0x4000 Encapsulation: ENET2
    Bandwidth: 1000mbps
    Routing Instance: default-switch Bridging Domain: vl214
    Input packets : 4
    Output packets: 55
    Protocol inet, MTU: 1582
      Flags: Sendbcast-pkt-to-re, User-MTU
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.101.16.128/25, Local: 10.101.16.129, Broadcast: 10.101.16.255
    Protocol multiservice, MTU: 1582

  Logical interface irb.1170 (Index 338) (SNMP ifIndex 630)
    Flags: Up SNMP-Traps 0x4000 Encapsulation: ENET2
    Bandwidth: 1000mbps
    Routing Instance: default-switch Bridging Domain: vl1170
    Input packets : 18
    Output packets: 44
    Protocol inet, MTU: 1582
      Flags: Sendbcast-pkt-to-re, User-MTU
      Addresses, Flags: Is-Preferred Is-Primary
        Destination: 10.117.170/24, Local: 10.117.170.3, Broadcast: 10.117.170.255
    Protocol multiservice, MTU: 1582

Physical interface: jsrv, Enabled, Physical link is Up
  Interface index: 135, SNMP ifIndex: 618
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Link type      : Full-Duplex
  Link flags     : None
  Current address: dc:38:e1:f8:fc:00, Hardware address: dc:38:e1:f8:fc:00
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

  Logical interface jsrv.1 (Index 323) (SNMP ifIndex 619)
    Flags: Up 0x24004000 Encapsulation: unknown
    Bandwidth: 1000mbps
    Routing Instance: None Bridging Domain: None
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: 1514
      Flags: Is-Primary
      Addresses, Flags: Primary Is-Default Is-Preferred Is-Primary
        Destination: 128/2, Local: 128.0.0.127, Broadcast: 191.255.255.255

Physical interface: lo0, Enabled, Physical link is Up
  Interface index: 6, SNMP ifIndex: 6
  Type: Loopback, MTU: Unlimited
  Device flags   : Present Running Loopback
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 32327
    Output packets: 32327

  Logical interface lo0.0 (Index 339) (SNMP ifIndex 16)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Flags: Sendbcast-pkt-to-re
      Addresses, Flags: Is-Default Is-Primary
        Local: 1.1.1.1

  Logical interface lo0.16384 (Index 320) (SNMP ifIndex 21)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 0
    Output packets: 0
    Protocol inet, MTU: Unlimited
      Addresses
        Local: 127.0.0.1

  Logical interface lo0.16385 (Index 321) (SNMP ifIndex 22)
    Flags: Down SNMP-Traps Encapsulation: Unspecified
    Input packets : 32323
    Output packets: 32323
    Protocol inet, MTU: Unlimited

Physical interface: lsi, Enabled, Physical link is Up
  Interface index: 4, SNMP ifIndex: 4
  Type: Software-Pseudo, Link-level type: LSI, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: mtun, Enabled, Physical link is Up
  Interface index: 65, SNMP ifIndex: 12
  Type: Multicast-GRE, Link-level type: GRE, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
    Input packets : 0
    Output packets: 0

Physical interface: pimd, Enabled, Physical link is Up
  Interface index: 26, SNMP ifIndex: 11
  Type: PIMD, Link-level type: PIM-Decapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pime, Enabled, Physical link is Up
  Interface index: 25, SNMP ifIndex: 10
  Type: PIME, Link-level type: PIM-Encapsulator, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
    Input packets : 0
    Output packets: 0

Physical interface: pip0, Enabled, Physical link is Up
  Interface index: 130, SNMP ifIndex: 503
  Type: Ethernet, Link-level type: Ethernet, MTU: 1514
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Current address: dc:38:e1:f8:03:b0, Hardware address: dc:38:e1:f8:03:b0
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: pp0, Enabled, Physical link is Up
  Interface index: 131, SNMP ifIndex: 504
  Type: PPPoE, Link-level type: PPPoE, MTU: 1532
  Device flags   : Present Running
  Interface flags: Point-To-Point SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None

Physical interface: tap, Enabled, Physical link is Up
  Interface index: 12, SNMP ifIndex: 7
  Type: Software-Pseudo, Link-level type: Interface-Specific, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

Physical interface: vtep, Enabled, Physical link is Up
  Interface index: 133, SNMP ifIndex: 620
  Type: Software-Pseudo, Link-level type: VxLAN-Tunnel-Endpoint, MTU: Unlimited, Speed: Unlimited
  Device flags   : Present Running
  Interface flags: SNMP-Traps
  Link type      : Full-Duplex
  Link flags     : None
  Last flapped   : Never
    Input packets : 0
    Output packets: 0

