Interface Ethernet1 detected 0 LLDP neighbors:

Interface Ethernet2 detected 0 LLDP neighbors:

Interface Ethernet3 detected 1 LLDP neighbors:

  Neighbor 0005.8671.f0c0/ge-0/0/15, age 4 seconds
  Discovered 12:58:59 ago; Last changed 12:58:59 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.f0c0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/15"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/15"
    - System Name: "sjc-ce01"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet4 detected 1 LLDP neighbors:

  Neighbor 0005.8671.9ec0/ge-0/0/15, age 3 seconds
  Discovered 12:58:55 ago; Last changed 12:58:55 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.9ec0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/15"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/15"
    - System Name: "sjc-ce02"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet5 detected 1 LLDP neighbors:

  Neighbor 0021.00ca.3c6d/Ethernet3, age 4 seconds
  Discovered 12:58:38 ago; Last changed 12:58:38 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0021.00ca.3c6d
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc101"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.21
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet6 detected 1 LLDP neighbors:

  Neighbor 0001.0032.2f20/Ethernet3, age 8 seconds
  Discovered 12:58:38 ago; Last changed 12:58:38 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0001.0032.2f20
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc102"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.22
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet7 detected 1 LLDP neighbors:

  Neighbor 0002.0014.2858/Ethernet3, age 2 seconds
  Discovered 12:58:44 ago; Last changed 12:58:44 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0002.0014.2858
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc103"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.23
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet8 detected 1 LLDP neighbors:

  Neighbor 0003.00e8.b231/Ethernet3, age 11 seconds
  Discovered 12:58:39 ago; Last changed 12:58:39 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0003.00e8.b231
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc104"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.24
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet9 detected 1 LLDP neighbors:

  Neighbor 0004.006e.c44a/Ethernet3, age 11 seconds
  Discovered 12:58:41 ago; Last changed 12:58:41 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0004.006e.c44a
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc105"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.25
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet10 detected 1 LLDP neighbors:

  Neighbor 0005.0061.bc7c/Ethernet3, age 7 seconds
  Discovered 12:58:39 ago; Last changed 12:58:39 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.0061.bc7c
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc106"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.26
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet11 detected 1 LLDP neighbors:

  Neighbor 0006.002d.192b/Ethernet3, age 23 seconds
  Discovered 12:58:53 ago; Last changed 12:58:53 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0006.002d.192b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc107"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.27
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet12 detected 1 LLDP neighbors:

  Neighbor 0007.0004.c3f6/Ethernet3, age 10 seconds
  Discovered 12:58:37 ago; Last changed 12:58:37 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0007.0004.c3f6
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc108"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.28
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet13 detected 1 LLDP neighbors:

  Neighbor 0008.00fb.b12f/Ethernet3, age 3 seconds
  Discovered 12:58:59 ago; Last changed 12:58:59 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0008.00fb.b12f
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc109"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.29
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet14 detected 1 LLDP neighbors:

  Neighbor 0009.0028.ba81/Ethernet3, age 9 seconds
  Discovered 12:58:42 ago; Last changed 12:58:42 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0009.0028.ba81
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc110"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.30
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet15 detected 1 LLDP neighbors:

  Neighbor 0010.008c.3be2/Ethernet3, age 30 seconds
  Discovered 12:59:00 ago; Last changed 12:59:00 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0010.008c.3be2
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc111"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.31
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet16 detected 1 LLDP neighbors:

  Neighbor 0011.004b.3d44/Ethernet3, age 5 seconds
  Discovered 12:58:33 ago; Last changed 12:58:33 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0011.004b.3d44
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc112"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.32
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet17 detected 0 LLDP neighbors:

Interface Ethernet18 detected 1 LLDP neighbors:

  Neighbor 0019.0089.ce11/Ethernet18, age 19 seconds
  Discovered 12:58:51 ago; Last changed 12:58:51 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0019.0089.ce11
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet18"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-dist04"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.104
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet19 detected 0 LLDP neighbors:

Interface Management1 detected 0 LLDP neighbors:

