Interface Ethernet1 detected 0 LLDP neighbors:

Interface Ethernet2 detected 0 LLDP neighbors:

Interface Ethernet3 detected 1 LLDP neighbors:

  Neighbor 0005.8671.f0c0/ge-0/0/16, age 3 seconds
  Discovered 22:58:22 ago; Last changed 22:58:22 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.f0c0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/16"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/16"
    - System Name: "sjc-ce01"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet4 detected 1 LLDP neighbors:

  Neighbor 0005.8671.9ec0/ge-0/0/16, age 2 seconds
  Discovered 22:58:22 ago; Last changed 22:58:22 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.9ec0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/16"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/16"
    - System Name: "sjc-ce02"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet5 detected 1 LLDP neighbors:

  Neighbor 0009.00cb.6f3f/Ethernet4, age 28 seconds
  Discovered 22:58:03 ago; Last changed 22:58:03 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0009.00cb.6f3f
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc001"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.1
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet6 detected 1 LLDP neighbors:

  Neighbor 0010.0017.2cd3/Ethernet4, age 5 seconds
  Discovered 22:58:06 ago; Last changed 22:58:06 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0010.0017.2cd3
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc002"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.2
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet7 detected 1 LLDP neighbors:

  Neighbor 0011.00fb.258e/Ethernet4, age 11 seconds
  Discovered 22:58:17 ago; Last changed 22:58:17 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0011.00fb.258e
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc003"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.3
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet8 detected 1 LLDP neighbors:

  Neighbor 0012.0098.b0ef/Ethernet4, age 24 seconds
  Discovered 22:58:25 ago; Last changed 22:58:25 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0012.0098.b0ef
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc004"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.4
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet9 detected 1 LLDP neighbors:

  Neighbor 0013.00fa.87ce/Ethernet4, age 14 seconds
  Discovered 22:58:10 ago; Last changed 22:58:10 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0013.00fa.87ce
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc005"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.5
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet10 detected 1 LLDP neighbors:

  Neighbor 0014.0026.baca/Ethernet4, age 16 seconds
  Discovered 22:58:16 ago; Last changed 22:58:16 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0014.0026.baca
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc006"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.6
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet11 detected 1 LLDP neighbors:

  Neighbor 0015.00c4.990b/Ethernet4, age 15 seconds
  Discovered 22:58:19 ago; Last changed 22:58:19 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0015.00c4.990b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc007"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.7
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet12 detected 1 LLDP neighbors:

  Neighbor 0016.00c9.a95b/Ethernet4, age 13 seconds
  Discovered 22:58:08 ago; Last changed 22:58:08 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0016.00c9.a95b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc008"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.8
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet13 detected 1 LLDP neighbors:

  Neighbor 0017.0060.2299/Ethernet4, age 26 seconds
  Discovered 22:58:02 ago; Last changed 22:58:02 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0017.0060.2299
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc009"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.9
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet14 detected 1 LLDP neighbors:

  Neighbor 0018.00b5.f88f/Ethernet4, age 7 seconds
  Discovered 22:57:58 ago; Last changed 22:57:58 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0018.00b5.f88f
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc010"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.10
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet15 detected 1 LLDP neighbors:

  Neighbor 0019.0060.a237/Ethernet4, age 11 seconds
  Discovered 22:58:08 ago; Last changed 22:58:08 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0019.0060.a237
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc011"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.11
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet16 detected 1 LLDP neighbors:

  Neighbor 0020.009c.da72/Ethernet4, age 12 seconds
  Discovered 22:58:09 ago; Last changed 22:58:09 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0020.009c.da72
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet4"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc012"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.12
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet17 detected 0 LLDP neighbors:

Interface Ethernet18 detected 1 LLDP neighbors:

  Neighbor 0016.00fa.4e3a/Ethernet18, age 0 seconds
  Discovered 22:58:19 ago; Last changed 22:58:19 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0016.00fa.4e3a
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet18"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-dist01"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.101
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet19 detected 0 LLDP neighbors:

Interface Management1 detected 0 LLDP neighbors:

