Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  Internet address is 10.100.0.28/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     36941 packets input, 3253793 bytes
     Received 1 broadcasts, 49 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     107943 packets output, 26968367 bytes
     Sent 11 broadcasts, 40106 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41 packets input, 2624 bytes
     Received 0 broadcasts, 41 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40114 packets output, 7259463 bytes
     Sent 0 broadcasts, 40114 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  Internet address is 10.115.5.2/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     299350 packets input, 42760934 bytes
     Received 958 broadcasts, 297786 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     209340 packets output, 23959639 bytes
     Sent 24 broadcasts, 207431 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  Internet address is 10.115.5.4/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     299562 packets input, 42799962 bytes
     Received 964 broadcasts, 297931 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     208813 packets output, 23726729 bytes
     Sent 19 broadcasts, 206166 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0018 (bia 0016.0000.0018)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41358 packets input, 7374190 bytes
     Received 6 broadcasts, 41005 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10142313 packets output, 837151321 bytes
     Sent 801911 broadcasts, 9340151 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.001b (bia 0016.0000.001b)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40940 packets input, 7341890 bytes
     Received 12 broadcasts, 40928 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10142538 packets output, 837192461 bytes
     Sent 801914 broadcasts, 9340140 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.001f (bia 0016.0000.001f)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41027 packets input, 7346217 bytes
     Received 13 broadcasts, 41014 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10140460 packets output, 836929601 bytes
     Sent 801850 broadcasts, 9338436 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0023 (bia 0016.0000.0023)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41555 packets input, 7405430 bytes
     Received 42 broadcasts, 41513 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10139527 packets output, 836825372 bytes
     Sent 801823 broadcasts, 9337596 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0025 (bia 0016.0000.0025)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     2339217 packets input, 248980904 bytes
     Received 172 broadcasts, 40619 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     12439234 packets output, 1077691132 bytes
     Sent 801692 broadcasts, 9338565 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0027 (bia 0016.0000.0027)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40795 packets input, 7315945 bytes
     Received 12 broadcasts, 40783 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10140595 packets output, 836991213 bytes
     Sent 801849 broadcasts, 9338558 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.002a (bia 0016.0000.002a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41311 packets input, 7375424 bytes
     Received 18 broadcasts, 41293 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10141846 packets output, 837145739 bytes
     Sent 801911 broadcasts, 9339822 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet12 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.002c (bia 0016.0000.002c)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41446 packets input, 7388655 bytes
     Received 27 broadcasts, 41061 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10140467 packets output, 836967163 bytes
     Sent 801844 broadcasts, 9338369 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet13 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.002f (bia 0016.0000.002f)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     41151 packets input, 7369283 bytes
     Received 28 broadcasts, 41123 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10140184 packets output, 836941913 bytes
     Sent 801855 broadcasts, 9338221 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet14 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0032 (bia 0016.0000.0032)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40782 packets input, 7327741 bytes
     Received 11 broadcasts, 40752 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10142257 packets output, 837186923 bytes
     Sent 801905 broadcasts, 9340178 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet15 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0034 (bia 0016.0000.0034)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40993 packets input, 7341910 bytes
     Received 3 broadcasts, 40990 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10142194 packets output, 837179607 bytes
     Sent 801914 broadcasts, 9340167 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet16 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0037 (bia 0016.0000.0037)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:06:43 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     40973 packets input, 7335524 bytes
     Received 3 broadcasts, 40970 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     10142234 packets output, 837186421 bytes
     Sent 801913 broadcasts, 9340208 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet17 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     39 packets input, 2496 bytes
     Received 0 broadcasts, 39 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40111 packets output, 7299365 bytes
     Sent 0 broadcasts, 40111 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.003a (bia 0016.0000.003a)
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     2144453 packets input, 214594806 bytes
     Received 400779 broadcasts, 1725553 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     8074649 packets output, 635186809 bytes
     Sent 401136 broadcasts, 7654094 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet19 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.00fa.4e3a
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 6 minutes, 5 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     39 packets input, 2496 bytes
     Received 0 broadcasts, 39 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40111 packets output, 7299424 bytes
     Sent 0 broadcasts, 40111 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Loopback0 is up, line protocol is up (connected)
  Hardware is Loopback
  Internet address is 10.117.255.101/32
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 65535 bytes
  Up 13 days, 21 hours, 51 minutes, 21 seconds
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0016.0000.0004 (bia 0016.0000.0004)
  Internet address is 10.117.38.71/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 2 minutes
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     40132 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Vlan1101 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.101.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 21 seconds
Vlan1102 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.102.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 21 seconds
Vlan1103 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.103.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1104 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.104.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1105 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.105.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1106 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.106.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1107 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.107.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1108 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.108.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1109 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.109.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
Vlan1110 is up, line protocol is up (connected)
  Hardware is Vlan, address is 0016.00fa.4e3a (bia 0016.00fa.4e3a)
  Internet address is 10.117.110.2/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 51 minutes, 20 seconds
