Ethernet1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  Internet address is 10.100.0.18/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     57568 packets input, 4860490 bytes
     Received 1 broadcasts, 46 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     229492 packets output, 49925789 bytes
     Sent 2 broadcasts, 120208 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     169650 packets input, 191268434 bytes
     Received 1 broadcasts, 169420 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     182542 packets output, 103997037 bytes
     Sent 1 broadcasts, 182468 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet2.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.12/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet3 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     176945 packets input, 191902502 bytes
     Received 0 broadcasts, 176286 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     256630 packets output, 207474190 bytes
     Sent 3 broadcasts, 256463 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet3.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.20/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet4 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     179675 packets input, 192599868 bytes
     Received 0 broadcasts, 179019 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     259383 packets output, 207588391 bytes
     Sent 3 broadcasts, 259216 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet4.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.28/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet5 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     180024 packets input, 192841303 bytes
     Received 2 broadcasts, 179358 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     259523 packets output, 207601775 bytes
     Sent 2 broadcasts, 259355 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet5.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.36/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet6 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     173672 packets input, 191901892 bytes
     Received 0 broadcasts, 173013 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     253294 packets output, 206763026 bytes
     Sent 3 broadcasts, 253127 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet6.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.44/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 47 seconds
Ethernet7 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     174538 packets input, 192035113 bytes
     Received 1 broadcasts, 173878 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     254253 packets output, 206906053 bytes
     Sent 2 broadcasts, 254085 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet7.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.52/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet8 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     179320 packets input, 193001353 bytes
     Received 0 broadcasts, 178619 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     259255 packets output, 208687433 bytes
     Sent 3 broadcasts, 259058 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet8.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.60/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 45 seconds
Ethernet9 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     76471 packets input, 62559982 bytes
     Received 0 broadcasts, 76471 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     240438 packets output, 204829454 bytes
     Sent 0 broadcasts, 240438 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet9.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.66/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet10 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     180608 packets input, 193510292 bytes
     Received 0 broadcasts, 179949 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     260554 packets output, 208984339 bytes
     Sent 3 broadcasts, 260375 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet10.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.76/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 44 seconds
Ethernet11 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     174545 packets input, 192103424 bytes
     Received 0 broadcasts, 173883 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     254195 packets output, 207046773 bytes
     Sent 3 broadcasts, 254028 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet11.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.84/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet12 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     174129 packets input, 191977857 bytes
     Received 0 broadcasts, 173470 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     253667 packets output, 206850605 bytes
     Sent 3 broadcasts, 253500 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet12.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.92/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet13 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     177074 packets input, 192862402 bytes
     Received 1 broadcasts, 176414 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     256670 packets output, 208100161 bytes
     Sent 3 broadcasts, 256490 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet13.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.100/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet14 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     177908 packets input, 193345456 bytes
     Received 1 broadcasts, 177248 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     257407 packets output, 208144098 bytes
     Sent 2 broadcasts, 257221 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet14.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.108/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 42 seconds
Ethernet15 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     797267 packets input, 948610485 bytes
     Received 10 broadcasts, 796505 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     741428 packets output, 863489109 bytes
     Sent 13 broadcasts, 740648 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet15.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.0/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet15.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.4/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet15.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.8/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 42 seconds
Ethernet15.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.12/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 42 seconds
Ethernet15.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.16/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 42 seconds
Ethernet16 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0000.0045 (bia 0002.0000.0045)
  Member of Port-Channel12
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters 13 days, 22:02:02 ago
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     434768 packets input, 55961139 bytes
     Received 1268 broadcasts, 433384 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1321929 packets output, 175817443 bytes
     Sent 0 broadcasts, 1321929 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet17 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0000.0046 (bia 0002.0000.0046)
  Member of Port-Channel13
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     1167623 packets input, 136351211 bytes
     Received 3887 broadcasts, 1163377 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1674971 packets output, 668720128 bytes
     Sent 10 broadcasts, 1670149 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     179889 packets input, 192700183 bytes
     Received 1 broadcasts, 179230 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     259438 packets output, 207576040 bytes
     Sent 2 broadcasts, 259271 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet18.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.1.4/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 43 seconds
Ethernet19 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0000.0048 (bia 0002.0000.0048)
  Member of Port-Channel13
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     335597 packets input, 44233471 bytes
     Received 905 broadcasts, 334569 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1632316 packets output, 608151372 bytes
     Sent 5 broadcasts, 1626320 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet20 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0000.0049 (bia 0002.0000.0049)
  Member of Port-Channel12
  Ethernet MTU 9214 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     1068508 packets input, 125669230 bytes
     Received 3538 broadcasts, 1064636 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     1980194 packets output, 1100118534 bytes
     Sent 14 broadcasts, 1974464 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Ethernet21 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured, auto negotiation: off, uni-link: unknown
  Up 13 days, 22 hours, 1 minutes, 20 seconds
  Loopback Mode : None
  1 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (- with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (- with framing overhead), 0 packets/sec
     35 packets input, 2240 bytes
     Received 0 broadcasts, 35 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     120223 packets output, 21998427 bytes
     Sent 0 broadcasts, 120223 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Management1 is up, line protocol is up (connected)
  Hardware is Ethernet, address is 0002.0000.0035 (bia 0002.0000.0035)
  Internet address is 10.110.37.26/24
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes , BW 1000000 kbit
  Full-duplex, 1Gb/s, auto negotiation: on, uni-link: unknown
  Up 13 days, 1 hours, 29 seconds
  Loopback Mode : None
  5 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 0 bps (0.0% with framing overhead), 0 packets/sec
  5 minutes output rate 0 bps (0.0% with framing overhead), 0 packets/sec
     0 packets input, 0 bytes
     Received 0 broadcasts, 0 multicast
     0 runts, 0 giants
     0 input errors, 0 CRC, 0 alignment, 0 symbol, 0 input discards
     0 PAUSE input
     120207 packets output, 0 bytes
     Sent 0 broadcasts, 0 multicast
     0 output errors, 0 collisions
     0 late collision, 0 deferred, 0 output discards
     0 PAUSE output
Port-Channel12 is up, line protocol is up (connected)
  Hardware is Port-Channel, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured 
  Active members in this channel: 2
  ... Ethernet16 , Full-duplex, Unconfigured
  ... Ethernet20 , Full-duplex, Unconfigured
  Fallback mode is: off
  Up 13 days, 21 hours, 49 minutes, 35 seconds
  2 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 1.22 kbps (- with framing overhead), 1 packets/sec
  5 minutes output rate 8.51 kbps (- with framing overhead), 3 packets/sec
     1503190 packets input, 181623873 bytes
     Received 4806 broadcasts, 1497934 multicast
     0 input errors, 0 input discards
     3302021 packets output, 1275921613 bytes
     Sent 14 broadcasts, 3296291 multicast
     0 output errors, 0 output discards
Port-Channel12.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.96/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel12.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.100/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel12.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.104/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel12.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.108/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel12.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.112/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel13 is up, line protocol is up (connected)
  Hardware is Port-Channel, address is 0002.0044.63ef
  IP MTU 1500 bytes
  Full-duplex, Unconfigured 
  Active members in this channel: 2
  ... Ethernet17 , Full-duplex, Unconfigured
  ... Ethernet19 , Full-duplex, Unconfigured
  Fallback mode is: off
  Up 13 days, 21 hours, 49 minutes, 35 seconds
  2 link status changes since last clear
  Last clearing of "show interface" counters never
  5 minutes input rate 1.22 kbps (- with framing overhead), 1 packets/sec
  5 minutes output rate 8.73 kbps (- with framing overhead), 3 packets/sec
     1503132 packets input, 180577840 bytes
     Received 4792 broadcasts, 1497858 multicast
     0 input errors, 0 input discards
     3307185 packets output, 1276855493 bytes
     Sent 15 broadcasts, 3296368 multicast
     0 output errors, 0 output discards
Port-Channel13.101 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.128/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel13.102 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.132/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel13.103 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.136/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel13.104 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.140/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
Port-Channel13.105 is up, line protocol is up (connected)
  Hardware is Subinterface, address is 0002.0044.63ef
  Internet address is 10.110.2.144/31
  Broadcast address is 255.255.255.255
  Address determined by manual configuration
  IP MTU 1500 bytes
  Up 13 days, 21 hours, 49 minutes, 35 seconds
