
VRF name: default
Codes: C - connected, S - static, K - kernel, 
       O - OSPF, IA - OSPF inter area, E1 - OSPF external type 1,
       E2 - OSPF external type 2, N1 - OSPF NSSA external type 1,
       N2 - OSPF NSSA external type2, B I - iBGP, B E - eBGP,
       R - RIP, I - ISIS, A B - BGP Aggregate, A O - OSPF Summary,
       NG - Nexthop Group Static Route 

Gateway of last resort is not set

 K      0.0.0.0/8 is directly connected, <Internal>
 C      10.100.0.92/31 is directly connected, Ethernet1
 C      10.117.38.0/24 is directly connected, Management1
 C      10.117.255.9/32 is directly connected, Loopback0
 K      127.0.0.1/32 is directly connected, <Internal>
 K      127.0.0.0/8 is directly connected, <Internal>

