Interface Ethernet1 detected 0 LLDP neighbors:

Interface Ethernet2 detected 0 LLDP neighbors:

Interface Ethernet3 detected 1 LLDP neighbors:

  Neighbor 0005.8671.f0c0/ge-0/0/13, age 9 seconds
  Discovered 13:57:31 ago; Last changed 13:57:31 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.f0c0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/13"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/13"
    - System Name: "sjc-ce01"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet4 detected 1 LLDP neighbors:

  Neighbor 0005.8671.9ec0/ge-0/0/13, age 2 seconds
  Discovered 13:57:32 ago; Last changed 13:57:32 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0005.8671.9ec0
    - Port ID type: Interface name (5)
      Port ID     : "ge-0/0/13"
    - Time To Live: 40 seconds
    - Port Description: "ge-0/0/13"
    - System Name: "sjc-ce02"
    - System Description: "Juniper Networks, Inc. vmx , version 14.1R5.4 Build date: 2015-07-02 08:51:42 UTC "
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 MAC/PHY Configuration/Status
      Auto-negotiation       : Supported, Enabled
      Advertised Capabilities: Asymmetric and Symmetric PAUSE
                               10BASE-T (half-duplex)
                               10BASE-T (full-duplex)
                               100BASE-TX (half-duplex)
                               100BASE-TX (full-duplex)
                               1000BASE-X (half-duplex)
                               1000BASE-X (full-duplex)
                               1000BASE-T (full-duplex)
      Operational MAU Type   : Unknown (0)
    - IEEE802.3 Maximum Frame Size: 1514 bytes

Interface Ethernet5 detected 1 LLDP neighbors:

  Neighbor 0012.00dc.123b/Ethernet3, age 28 seconds
  Discovered 13:57:19 ago; Last changed 13:57:19 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0012.00dc.123b
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc201"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.41
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet6 detected 1 LLDP neighbors:

  Neighbor 0013.00bc.e2a7/Ethernet3, age 16 seconds
  Discovered 13:57:36 ago; Last changed 13:57:36 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0013.00bc.e2a7
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc202"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.42
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet7 detected 1 LLDP neighbors:

  Neighbor 0014.0077.6bd4/Ethernet3, age 7 seconds
  Discovered 13:57:29 ago; Last changed 13:57:29 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0014.0077.6bd4
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc203"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.43
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet8 detected 1 LLDP neighbors:

  Neighbor 0015.008c.ae7e/Ethernet3, age 3 seconds
  Discovered 13:57:25 ago; Last changed 13:57:25 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0015.008c.ae7e
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc204"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.44
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet9 detected 1 LLDP neighbors:

  Neighbor 0016.00ea.c417/Ethernet3, age 9 seconds
  Discovered 13:57:34 ago; Last changed 13:57:34 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0016.00ea.c417
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc205"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.45
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet10 detected 1 LLDP neighbors:

  Neighbor 0017.0010.8ef2/Ethernet3, age 18 seconds
  Discovered 13:57:11 ago; Last changed 13:57:11 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0017.0010.8ef2
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc206"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.46
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet11 detected 1 LLDP neighbors:

  Neighbor 0018.007c.a014/Ethernet3, age 27 seconds
  Discovered 13:57:26 ago; Last changed 13:57:26 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0018.007c.a014
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc207"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.47
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet12 detected 1 LLDP neighbors:

  Neighbor 0019.007b.3604/Ethernet3, age 25 seconds
  Discovered 13:57:22 ago; Last changed 13:57:22 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0019.007b.3604
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc208"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.48
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet13 detected 1 LLDP neighbors:

  Neighbor 0020.00d7.c230/Ethernet3, age 12 seconds
  Discovered 13:57:27 ago; Last changed 13:57:27 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0020.00d7.c230
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc209"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.49
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet14 detected 1 LLDP neighbors:

  Neighbor 0021.0089.c0dd/Ethernet3, age 22 seconds
  Discovered 13:57:18 ago; Last changed 13:57:18 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0021.0089.c0dd
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc210"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.50
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet15 detected 1 LLDP neighbors:

  Neighbor 0001.00a1.1d53/Ethernet3, age 27 seconds
  Discovered 13:57:25 ago; Last changed 13:57:25 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0001.00a1.1d53
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc211"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.51
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet16 detected 1 LLDP neighbors:

  Neighbor 0002.00f6.e819/Ethernet3, age 30 seconds
  Discovered 13:57:29 ago; Last changed 13:57:29 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0002.00f6.e819
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet3"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-acc212"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.52
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet17 detected 0 LLDP neighbors:

Interface Ethernet18 detected 1 LLDP neighbors:

  Neighbor 0021.0015.7349/Ethernet18, age 3 seconds
  Discovered 13:57:25 ago; Last changed 13:57:25 ago
    - Chassis ID type: MAC address (4)
      Chassis ID     : 0021.0015.7349
    - Port ID type: Interface name (5)
      Port ID     : "Ethernet18"
    - Time To Live: 120 seconds
    - System Name: "sjc-dc12-dist06"
    - System Description: "Arista Networks EOS version 4.15.0F running on an Arista Networks vEOS"
    - System Capabilities : Bridge, Router
      Enabled Capabilities: Bridge, Router
    - Management Address Subtype: IPv4 (1)
      Management Address        : 10.117.255.106
      Interface Number Subtype  : ifIndex (2)
      Interface Number          : 5000000
      OID String                : 
    - IEEE802.1 Port VLAN ID: 1
    - IEEE802.1/IEEE802.3 Link Aggregation
      Link Aggregation Status: Capable, Disabled (0x01)
      Port ID                : 0
    - IEEE802.3 Maximum Frame Size: 9236 bytes

Interface Ethernet19 detected 0 LLDP neighbors:

Interface Management1 detected 0 LLDP neighbors:

