CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl6/conf/instr/spect/uxnmr.info
Date         : Wed May  2 15:39:14 2018
Release      : TopSpin 3.5 pl 6
Installed in : /opt/topspin3.5pl6
Host         : av499
OS           : CentOS Linux release 7.4.1708 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 500 NMR spectrometer
1H-frequency : 499.92 MHz
Description  : AV III 500 HD Uni Koeln
Bruker Order : 10232140
Configured in: av499:/opt/topspin3.5pl6/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.91
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/05463 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.4 REC-1  AQS RXAD/2 600 Z130588/3004 ECL 00.04
     3   0x34 0xd6   0x1        X  5.2 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  3.3 SGU-1  AQS SGU/3 600 (2CH) Z117129/03419 ECL 03.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345098_0372 W1345098/0372 ECL 31:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAXH500/100 E 200-600MHZ INR: W1345098/0372 ECL 31
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/005729 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011732 ECL 60
LTRX Z109889/00987 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00987 ECL 03.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20160329
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00987 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03547 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03940 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Prodigy Control Unit: LNP PRODIGY UNIT Z127349/465
- TCP/IP address   = 149.236.99.93

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: BACS2_H15000-01_903
- TCP/IP address   = 149.236.99.119

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.3%/0.3deg, reflection meter)
                PN=Z103204, SN=00872 from 20160930
    Module  2 : 2H
                PN=Z003472, SN=01716 from 20161006
    Module  3 : XBB19F 2HS
                PN=Z003505, SN=01965 from 20161006
    Module  4 : 13C
                PN=Z003523, SN=00448 from 20160608
    Module  5 : 15N
                PN=Z003529, SN=00440 from 20160628



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH500/100 E 200-600MHZ INR W1345098/0372 at TCP/IP 149.236.99.92)
SGU1 AUX  output -> input 1 of transmitter 2 (BSMS/2 LOCK TRANSCEIVER 500 Z109889/00987 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH500/100 E 200-600MHZ INR W1345098/0372 at TCP/IP 149.236.99.92)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH500/100 E 200-600MHZ INR W1345098/0372 at TCP/IP 149.236.99.92:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1

transmitter 2 = BSMS/2 LOCK TRANSCEIVER 500 Z109889/00987 at TCP/IP 149.236.99.20:
- amplifier 2H-5W uses blanking 7


