CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Tue Feb 24 14:06:24 2015
Release      : TOPSPIN Version 3.2-pl6
Installed in : C:/Bruker/TopSpin3.2
Host         : BRUKER600
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5620 @ 2.40GHz (8 cores at 2394 MHz)
User         : BrukerUser
Description  : AV(2)600
Location     : Building 227 Room B139
System       : Avance-AV NMR spectrometer
1H-frequency : 600.13 MHz
Order Number : BH050005
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 3 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 4 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/03046 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 131205

Gcu: GCU3_SlowIF

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/636 ECL 04.04
     3   0x34 0xc0   0x1        X  0.4 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x18   0x4    BH  S  5.0 SGU-1  AQS SGU600 Z003642/01970 ECL 5.0
     5   0x25 0x18   0x4    BH  S  3.0 SGU-2  AQS SGU600 Z003831/01984 ECL 3.0
     6   0x26 0x18   0x4    BH  S  3.0 SGU-3  AQS SGU600 Z003831/01884 ECL 3.0
     8   0x3c  0x4     0        Y  1.0 ROUT-1 Avance Router 3/5
    21   0x21  0xa     0        P  1.0 PSD-1  Power Supply Distribution Board
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      300    N  (V=ff) BLAXH 300/100 W1345062/355/20050420
   2      1         2       1H      100    N  (-""-) BLAXH 300/100 W1345062/355/20050420
   3      2         1        X      300    N  (V=ff) BLAX 300 W1345069/699/20000509
   4      3         1       2H       20    N         BSMS 2HTX -/-/-



- Type: BSMS/1
- absolute lockshift frequency =  12123609 Hz
- 2HTX Amplifier: connected to router output 4
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Bruker Automatic Changer: device connected to spect:/dev/tty07
- Capacity: 60 holders
- Firmware: 20120928
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - BACS2_H15000-01_657: at TCP/IP address 149.236.99.54


Lock: device connected to spect:/dev/tty03

Eurotherm VTU: device connected to spect:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00365 from 20050110
    Module  2 : XBB19F 2HS
                 PN=Z003506, SN=00390 from 20050308
    Module  3 : 2H
                 PN=Z003473, SN=00369 from 20050202


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



