! Command: show running-config
! device: sjc-dc12-dist04 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-dist04
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1131-1140 priority 8192
!
!
no aaa root
!
!
vlan 1131-1140
!
vrf definition ECOMM-2-PROD
   rd 2:101
!
interface Ethernet1
   no switchport
   ip address 10.100.0.22/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   no switchport
   vrf forwarding ECOMM-2-PROD
   ip address 10.115.5.12/31
!
interface Ethernet4
   no switchport
   vrf forwarding ECOMM-2-PROD
   ip address 10.115.5.20/31
!
interface Ethernet5
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet6
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet7
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet8
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet9
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet10
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet11
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet12
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet13
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet14
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet15
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet16
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   switchport trunk allowed vlan 1131-1140
   switchport mode trunk
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.117.255.104/32
!
interface Management1
   ip address 10.117.38.74/24
!
interface Vlan1131
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.131.3/24
   ip virtual-router address 10.117.131.1
!
interface Vlan1132
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.132.3/24
   ip virtual-router address 10.117.132.1
!
interface Vlan1133
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.133.3/24
   ip virtual-router address 10.117.133.1
!
interface Vlan1134
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.134.3/24
   ip virtual-router address 10.117.134.1
!
interface Vlan1135
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.135.3/24
   ip virtual-router address 10.117.135.1
!
interface Vlan1136
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.136.3/24
   ip virtual-router address 10.117.136.1
!
interface Vlan1137
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.137.3/24
   ip virtual-router address 10.117.137.1
!
interface Vlan1138
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.138.3/24
   ip virtual-router address 10.117.138.1
!
interface Vlan1139
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.139.3/24
   ip virtual-router address 10.117.139.1
!
interface Vlan1140
   vrf forwarding ECOMM-2-PROD
   ip address 10.117.140.3/24
   ip virtual-router address 10.117.140.1
!
ip virtual-router mac-address 00:1c:73:00:00:02
!
ip routing
ip routing vrf ECOMM-2-PROD
!
router ospf 1 vrf ECOMM-2-PROD
   router-id 10.117.255.104
   network 0.0.0.0/0 area 0.0.0.0
   max-lsa 12000
!
!
end
