! Command: show running-config
! device: sjc-dc12-dist08 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-dist08
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1181-1190 priority 8192
!
!
no aaa root
!
!
vlan 1181-1190
!
vrf definition CORP-EXTRANET1
   rd 2:109
!
interface Ethernet1
   no switchport
   ip address 10.100.0.32/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   no switchport
   vrf forwarding CORP-EXTRANET1
   ip address 10.115.5.24/31
!
interface Ethernet4
   no switchport
   vrf forwarding CORP-EXTRANET1
   ip address 10.115.5.32/31
!
interface Ethernet5
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet6
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet7
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet8
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet9
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet10
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet11
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet12
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet13
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet14
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet15
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet16
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   switchport trunk allowed vlan 1181-1190
   switchport mode trunk
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.117.255.108/32
!
interface Management1
   ip address 10.117.38.78/24
!
interface Vlan1181
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.181.3/24
   ip virtual-router address 10.117.181.1
!
interface Vlan1182
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.182.3/24
   ip virtual-router address 10.117.182.1
!
interface Vlan1183
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.183.3/24
   ip virtual-router address 10.117.183.1
!
interface Vlan1184
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.184.3/24
   ip virtual-router address 10.117.184.1
!
interface Vlan1185
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.185.3/24
   ip virtual-router address 10.117.185.1
!
interface Vlan1186
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.186.3/24
   ip virtual-router address 10.117.186.1
!
interface Vlan1187
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.187.3/24
   ip virtual-router address 10.117.187.1
!
interface Vlan1188
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.188.3/24
   ip virtual-router address 10.117.188.1
!
interface Vlan1189
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.189.3/24
   ip virtual-router address 10.117.189.1
!
interface Vlan1190
   vrf forwarding CORP-EXTRANET1
   ip address 10.117.190.3/24
   ip virtual-router address 10.117.190.1
!
ip virtual-router mac-address 00:1c:73:00:00:04
!
ip routing
ip routing vrf CORP-EXTRANET1
!
router ospf 1 vrf CORP-EXTRANET1
   router-id 10.117.255.108
   network 0.0.0.0/0 area 0.0.0.0
   max-lsa 12000
!
!
end
