## Last commit: 2019-01-11 04:03:33 PST by testuser
version 15.1R2.9;
system {
    host-name ex01;
    domain-name dc.local.forwardnetworks.com;
    time-zone America/Los_Angeles;
    name-server {
        10.128.64.1;
    }
    services {
        ssh {
            protocol-version v2;
        }
    }
    ntp {
        server 216.229.4.66;
    }
}
interfaces {
    ge-1/0/0 {
        enable;
        vlan-tagging;
        mtu 1600;
        unit 0 {
            family ethernet-switching {
                interface-mode trunk;
                vlan {
                    members [ 30 1170 ];
                }
            }
        }
    }
    ge-1/0/1 {
        enable;
        vlan-tagging;
        mtu 1600;
        unit 0 {
            family ethernet-switching {
                interface-mode trunk;
                vlan {
                    members [ 214 1170 ];
                }
            }
        }
    }
    ge-1/0/2 {
        enable;
        unit 0 {
            description test_port;
            family inet {
                address 192.168.10.1/24;
            }
        }
    }
    ge-1/0/3 {
        enable;
    }
    fxp0 {
        unit 0 {
            family inet {
                address 10.128.64.10/24;
            }
        }
    }
    irb {
        unit 30 {
            family inet {
                address 192.168.59.2/24;
            }
        }
        unit 214 {
            family inet {
                mtu 1600;
                address 10.101.16.129/25;
            }
        }
        unit 1170 {
            family inet {
                mtu 1600;
                address 10.117.170.3/24;
            }
        }
    }
    lo0 {
        unit 0 {
            family inet {
                address 1.1.1.1/32;
            }
        }
    }
}
routing-options {
    static {
        route 0.0.0.0/0 {
            next-hop 10.128.64.1;
            retain;
            no-readvertise;
        }
    }
}
protocols {
    ospf {
        traceoptions {
            file ospf size 5m world-readable;
            flag hello detail;
        }
        area 0.0.0.0 {
            interface all {
                hello-interval 1;
            }
        }
    }
    lldp {
        interface all;
    }
}
vlans {
    vl1170 {
        vlan-id 1170;
        l3-interface irb.1170;
    }
    vl214 {
        vlan-id 214;
        l3-interface irb.214;
    }
    vl30 {
        vlan-id 30;
        l3-interface irb.30;
    }
}


