! Command: show running-config
! device: sjc-dc12-dist01 (vEOS, EOS-4.15.0F)
!
! boot system flash:/vEOS-lab.swi
!
transceiver qsfp default-mode 4x10G
!
hostname sjc-dc12-dist01
!
spanning-tree mode rapid-pvst
spanning-tree vlan 1101-1110 priority 4096
!
!
no aaa root
!
!
vlan 1101-1110
!
vrf definition ECOMM-2-QA
   rd 2:102
!
interface Ethernet1
   no switchport
   ip address 10.100.0.28/31
!
interface Ethernet2
   no switchport
!
interface Ethernet3
   no switchport
   vrf forwarding ECOMM-2-QA
   ip address 10.115.5.2/31
!
interface Ethernet4
   no switchport
   vrf forwarding ECOMM-2-QA
   ip address 10.115.5.4/31
!
interface Ethernet5
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet6
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet7
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet8
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet9
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet10
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet11
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet12
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet13
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet14
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet15
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet16
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet17
   no switchport
!
interface Ethernet18
   switchport trunk allowed vlan 1101-1110
   switchport mode trunk
!
interface Ethernet19
   no switchport
!
interface Loopback0
   ip address 10.117.255.101/32
!
interface Management1
   ip address 10.117.38.71/24
!
interface Vlan1101
   vrf forwarding ECOMM-2-QA
   ip address 10.117.101.2/24
   ip virtual-router address 10.117.101.1
!
interface Vlan1102
   vrf forwarding ECOMM-2-QA
   ip address 10.117.102.2/24
   ip virtual-router address 10.117.102.1
!
interface Vlan1103
   vrf forwarding ECOMM-2-QA
   ip address 10.117.103.2/24
   ip virtual-router address 10.117.103.1
!
interface Vlan1104
   vrf forwarding ECOMM-2-QA
   ip address 10.117.104.2/24
   ip virtual-router address 10.117.104.1
!
interface Vlan1105
   vrf forwarding ECOMM-2-QA
   ip address 10.117.105.2/24
   ip virtual-router address 10.117.105.1
!
interface Vlan1106
   vrf forwarding ECOMM-2-QA
   ip address 10.117.106.2/24
   ip virtual-router address 10.117.106.1
!
interface Vlan1107
   vrf forwarding ECOMM-2-QA
   ip address 10.117.107.2/24
   ip virtual-router address 10.117.107.1
!
interface Vlan1108
   vrf forwarding ECOMM-2-QA
   ip address 10.117.108.2/24
   ip virtual-router address 10.117.108.1
!
interface Vlan1109
   vrf forwarding ECOMM-2-QA
   ip address 10.117.109.2/24
   ip virtual-router address 10.117.109.1
!
interface Vlan1110
   vrf forwarding ECOMM-2-QA
   ip address 10.117.110.2/24
   ip virtual-router address 10.117.110.1
!
ip virtual-router mac-address 00:1c:73:00:00:01
!
ip routing
ip routing vrf ECOMM-2-QA
!
router ospf 1 vrf ECOMM-2-QA
   router-id 10.117.255.101
   network 0.0.0.0/0 area 0.0.0.0
   max-lsa 12000
!
!
end
